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AUDIO


	WIRELESS PRO AUDIO	

	WiSpeak	
Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CCORE	CORE	WiSpeak CORE is the transmitter device that communicates with all the receiver devices to create a	495,80 €
WiSpeak wireless network, and takes the role of the Master Unit.
Its main functions are to pair and send audio contents to all the receivers. Includes 3 audio inputs (Euroblock, RCA, Bluetooth), remote port for a WPa-VOL panel and a MUTE port for external dry contact triggering. Managed by WiSpeak grip app.
Dimensions 225x120x40mm / 8.9”x4.7”x1.6”. Weight 0.8kg / 1.76 lb.
	629,67 €
	200 800 Ft
	255 016 Ft



	CTUBE3WH	TUBE	WiSpeak TUBE is a self-powered 3" lamp style loudspeaker with wireless audio reception and control	403,46 €
capabilities under the control of the Master unit, featuring an AUX output (Euroblock) and a installation system which is compatible with ceiling light rails. Dimensions (without accessories) Ø 96mm x 110mm /Ø 3,8" x 4,3" . Weight 0,8 kg / 1.76lb. White colour.
Delivered by units. Price per unit.
	512,39 €
	163 400 Ft
	207 518 Ft



	CTUBE3BK	TUBE	WiSpeak TUBE is a self-powered 3" lamp style loudspeaker with wireless audio reception and control	403,46 €
capabilities under the control of the Master unit, featuring an AUX output (Euroblock) and a installation system which is compatible with ceiling light rails. Dimensions (without accessories) Ø 96mm x 110mm /Ø 3,8" x 4,3" . Weight 0,8 kg / 1.76lb. Black colour. Delivered by units. Price per unit.
	512,39 €
	163 400 Ft
	207 518 Ft



	CCUBE5WH	CUBE	WiSpeak CUBE is a self-powered 5" loudspeaker cabinet with wireless audio reception and control	507,65 €
capabilities under the control of the Master unit, featuring an AUX output (Euroblock) and a installation system which is compatible with ceiling light rails. Alternatively, wall mount or desktop installation is as well possible by means of the included accessories. Dimensions (without accessories) 173x180x185 mm / 6,81" x 7,08" x 7,28". Weight 2,4kg / 5.29lb. White colour. Delivered by units. Price per unit.
	644,72 €
	205 600 Ft
	261 112 Ft



	CCUBE5BK	CUBE	WiSpeak CUBE is a self-powered 5" loudspeaker cabinet with wireless audio reception and control	507,65 €
capabilities under the control of the Master unit, featuring an AUX output (Euroblock) and a installation system which is compatible with ceiling light rails. Alternatively, wall mount or desktop installation is as well possible by means of the included accessories. Dimensions (without accessories) 173x180x185 mm / 6,81" x 7,08" x 7,28". Weight 2,4kg / 5.29lb. Black colour. Delivered by units. Price per unit.
	644,72 €
	205 600 Ft
	261 112 Ft



	CGLOBE5PDWH	GLOBE	WiSpeak GLOBE is a self-powered 2-way full range sphere loudspeaker cabinet with wireless audio	480,74 €
reception and control capabilities under the control of a WiSpeak CORE Master unit, featuring a pendant installation system. Includes a 5" woofer and a 1" silk dome tweeter. Dimensions (without accessories) Ø287mm x 331mm(H) / Ø11.3 in. x 13 in. (H). Weight 2.2 Kg / 4.85 lbs. White colour. Delivered by units. Price per unit.
	610,54 €
	194 700 Ft
	247 269 Ft



	CGLOBE5PDBK	GLOBE	WiSpeak GLOBE is a self-powered 2-way full range sphere loudspeaker cabinet with wireless audio	480,74 €
reception and control capabilities under the control of a WiSpeak CORE Master unit, featuring a pendant installation system. Includes a 5" woofer and a 1" silk dome tweeter. Dimensions (without accessories) Ø287mm x 331mm(H) / Ø11.3 in. x 13 in. (H). Weight 2.2 Kg / 4.85 lbs. Black colour.
Delivered by units. Price per unit.
	610,54 €
	194 700 Ft
	247 269 Ft



	CGLOBE5RMWH	GLOBE	WiSpeak GLOBE is a self-powered 2-way full range sphere loudspeaker cabinet with wireless audio	480,74 €
reception and control capabilities under the control of a WiSpeak CORE Master unit, featuring an installation system which is compatible with ceiling light rails. Includes a 5" woofer and a 1" silk dome tweeter. Dimensions (without accessories) Ø287mm x 331mm(H) / Ø11.3 in. x 13 in. (H). Weight 2.2 Kg
/ 4.85 lbs. White colour. Delivered by units. Price per unit.
	610,54 €
	194 700 Ft
	247 269 Ft



	CGLOBE5RMBK	GLOBE	WiSpeak GLOBE is a self-powered 2-way full range sphere loudspeaker cabinet with wireless audio	480,74 €
reception and control capabilities under the control of a WiSpeak CORE Master unit, featuring an installation system which is compatible with ceiling light rails. Includes a 5" woofer and a 1" silk dome tweeter. Dimensions (without accessories) Ø287mm x 331mm(H) / Ø11.3 in. x 13 in. (H). Weight 2.2 Kg
/ 4.85 lbs. Black colour. Delivered by units. Price per unit.
	610,54 €
	194 700 Ft
	247 269 Ft














	WiLD	

Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	NEW!
	CWILDTX
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	WiLD-TX
	WiLD-TX is the transmitter device that communicates with all the receiver devices to create a WiLD wireless network.2 audio inputs available: Analogue stereo, unbalanced. 2 x RCA connectors and Bluetooth®, class 1 (up to 25 meters range, maximum). Mute port and remote port (WPaVOL or compatible panel). Dimensions TBC. Weight TBC. Black colour. Delivered by units. Price per unit.
	330,12 €
	419,26 €
	133 700 Ft
	169 799 Ft



	NEW!
	CWILD14WH
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	WiLD-14
	WiLD-14 is a self-powered 4" lamp style loudspeaker with wireless audio reception under the control of the transmitter, featuring an installation system which is compatible with ceiling light rails. 4" woofer
+ 0,75" tweeter, 40W amplifier power output. Dimensions TBC. Weight TBC. White colour. Delivered by units. Price per unit.
	400,49 €
	508,63 €
	162 200 Ft
	205 994 Ft



	NEW!
	CWILD14BK
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	WiLD-14
	WiLD-14 is a self-powered 4" lamp style loudspeaker with wireless audio reception under the control of the transmitter, featuring an installation system which is compatible with ceiling light rails. 4" woofer
+ 0,75" tweeter, 40W amplifier power output. Dimensions TBC. Weight TBC. Black colour. Delivered by units. Price per unit.
	400,49 €
	508,63 €
	162 200 Ft
	205 994 Ft



	NEW!
	CWILDSB18BK
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	WiLD-SB18
	WiLD-SB18 is a compact self-powered 8" subwoofer with wireless audio reception under the control of the transmitter. 8" woofer. 100W Amplifier power output. Dimensions TBC. Weight TBC. Black colour. Delivered by units. Price per unit.
	801,73 €
	1 018,20 €
	324 700 Ft
	412 369 Ft


ACCESSORIES
Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF



	CTUBESMAWH	TUBE SMA	TUBESMA is a surface mount adapter to allow installing a TUBE or WiLD-14 unit in locations where	39,26 €
there is no available lighting rail.
	49,86 €
	15 900 Ft
	20 193 Ft



	CTUBESMABK	TUBE SMA	TUBESMA is a surface mount adapter to allow installing a TUBE or WiLD-14 unit in locations where	39,26 €
there is no available lighting rail.
	49,86 €
	15 900 Ft
	20 193 Ft



	SOUND SOURCES
	

	
	
	
	
	

	MICROPHONES
	
	
	
	

	
	
	
	
	

	Ref.	Name
	Nettó lista ár EUR
	Bruttó lista ár EUR
	Nettó lista ár HUF
	Bruttó lista ár HUF



	CEMHH1	eMHH1	Affordable handheld cardioid dynamic microphone, with a robust design that makes it ideal for voice	68,40 €
applications. It comes with a microphone stand adapter, 6 metres XLR-XLR cable and transport bag. Dimensions 185 x 50 x 50 mm. Weight 246 g.
	86,86 €
	27 700 Ft
	35 179 Ft



	CEMCN2	eMCN2	Condenser gooseneck cardioid microphone, with a perfect profile for message, speech and	115,56 €
conferencing applications. Total length 55 cm. It includes anti-pop wind-screen cover.
	146,76 €
	46 800 Ft
	59 436 Ft



	CEMBASE	eMBASE	Desktop connection base for the eMCN2 microphone, as well as for other microphones with standard	87,41 €
XLR connector. It includes ON / OFF switch that enables / disables the microphone signal. Dimensions 45 x 140 x 110 mm. Weight: 860g.
	111,01 €
	35 400 Ft
	44 958 Ft


AUDIO PLAYERS
Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF



	CPLAYERONE	PLAYER ONE	Compact audio player with a stereo output that can play music contents from local storage media	505,68 €
(USB/MicroSD card), Internet streams or digital sharing streams (DLNA and Airplay compatible). It includes Ethernet port, WiFi connection, USB and Micro-SD reader slots, front panel LCD display and local controls .Remote management by Ecler GALLERY, remote control by RePLAYER mobile app.
Dimensions 241 x 44 x 152mm (install 2 PLAYER ONE in 1RU with 1UHRMKIT accessory). Weight 680 g.
	642,21 €
	204 800 Ft
	260 096 Ft



	CPLAYERZERO	PLAYER ZERO	Compact audio player with a stereo output that can play music contents from local storage media	405,43 €
(USB/MicroSD card), Internet streams or digital sharing streams (DLNA and Airplay compatible). It includes Ethernet port, WiFi connection, USB and Micro-SD reader slots .Remote management by Ecler GALLERY, remote control by RePLAYER mobile app. Dimensions 126.5 x 44 x 132 mm / 4.98” x 1.73” x
5.19“. Weight 0.6 Kg / 1.32 lb
	514,90 €
	164 200 Ft
	208 534 Ft
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	CDUONTPLAYER	DUONET PLAYER	Double audio sound source that features full EclerNet compatibility (UCP control system,	1 085,68 €
WPNETTOUCH remote management, TP-NET protocol, etc.). It includes 2 independent stereo media players, each one being able to play Internet audio streams and local (USB/SD) or networked audio media. The device have 2 Euroblock line level balanced outputs, remote control, priority (messages, warnings) and 4 GPI ports to trigger events. Dimensions 482 x 44(1RU) x 250mm. Weight 4,2 kg
	1 378,81 €
	439 700 Ft
	558 419 Ft



	CESASBT	eSAS-BT	Stereo audio source including FM tuner, USB slot, SD slot and Bluetooth connection. It performs	278,02 €
unbalanced and balanced stereo audio outputs and headphones output (jack) with volume control in frontal panel. IR remote control, FM antenna, 2x RCA cables and rack-mount bracket included.
Dimensions 482 x 44(1RU) x 132mm. Weight 1,4 kg
	353,09 €
	112 600 Ft
	143 002 Ft



	INSTALLATION MIXERS
	

	
	
	
	
	

	INSTALLATION MIXERS
	
	
	
	

	
	
	
	
	

	Ref.	Name	SAM SERIES
	Nettó lista ár EUR
	Bruttó lista ár EUR
	Nettó lista ár HUF
	Bruttó lista ár HUF



	EOL
	CESAM702C
	eSAM702
	Installation audio mixer in standard rack format, featuring 6 MIC/LINE ST inputs, 1 LINE ST input, 1 main mix balanced output and one AUX/REC additional output. It includes a 3 band tone control section, Talkover (priority) function assignable to each MIC/LINE input over the mix bus, 18V phantom available for all mic inputs, ST/MONO mix switch and MUTE port for external dry contact triggering. Dimensions 482.6 x 44(1RU) x 120 mm. Weight 1,8 kg
	514,81 €
	653,81 €
	208 500 Ft
	264 795 Ft



	EOL
	CSAM612T
	SAM612T
	Installation audio mixer in standard rack format, featuring 6 MIC/LINE ST inputs + 1 ST MIX input and 1 stereo balanced output. Each input has a dedicated 3-band tone control and 18V phantom power for MIC inputs. Input 1 includes talkover (priority) function over the mix bus and additional front panel jack connector. Main output ST/MONO mode switch and MUTE port for external dry contact triggering.
Dimensions 482.6x44(1RU)x120 mm. Weight 2,0 kg
	594,07 €
	754,47 €
	240 600 Ft
	305 562 Ft


Ref.
Name
COMPACT SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CECOMPACT4BT	eCOMPACT4BT	Desktop/19" rack installation mixer. INS: 4 mic with switchable HP-filter and Phantom power 48V; 6	897,04 €
line ST; Bluetooth® connex; aux (mini-jack). OUTS: main balanced (XLR) with ST/mono switch; SUB OUT mono (XLR) with switchable LP-filter; alternative ALT (RCA); headphones (mini-Jack). 3 Band tone Ctrl and ALT OUT (alternative output) send per channel on all channels; Talkover (CH4) with mic input (combo) and USB charging port. It includes power supply and rack-mount kit.
	1 139,24 €
	363 300 Ft
	461 391 Ft


Ref.
Name
SAMI SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	NEW!
	CSAMI402
	SAMI-402
	Installation audio mixer in standard rack format, featuring 3 MIC/LINE ST inputs, 1 LINE ST input, 1 main mix balanced output and one AUX/REC additional output. It includes a 3 band tone control section, Talkover (priority) function assignable to each MIC/LINE input over the mix bus, 18V phantom power for all mic inputs, ST/MONO mix switch and MUTE port for external dry contact triggering.
Dimensions 482.6 x 44(1RU) x 120 mm. Weight 1,7 kg
	389,38 €
	494,52 €
	157 700 Ft
	200 279 Ft



	NEW!
	CSAMI603
	SAMI-603
	6 inputs and 3 outputs installation audio mixer. Inputs: 1x MIC, 4x MIC/LINE ST, 1x LINE ST. Outputs: 1x ST (A/B) and 1x MONO (C). A/B output can operates in ST/MONO mode. Each input can be routed to output A, B and/or C. It includes a 3 band tone control section, talkover (priority) function assignable to each input over the mix bus, ST/MONO mix switch for A/B output and MUTE port for external dry contact triggering. Dimensions 482.6x44(1RU)x120 mm. Weight 2,1 kg
	535,80 €
	680,47 €
	217 000 Ft
	275 590 Ft



	NEW!
	CSAMI612
	SAMI-612
	Installation audio mixer in standard rack format, featuring 6 MIC/LINE ST inputs + 1 ST MIX input and 1 stereo balanced output. Each input has a dedicated 3-band tone control and 18V phantom power for MIC inputs. Input 1 includes talkover (priority) function over the mix bus and additional front panel jack connector. Main output ST/MONO mode switch and MUTE port for external dry contact triggering. Dimensions 482.6x44(1RU)x120 mm. Weight 2,0 kg
	550,86 €
	699,60 €
	223 100 Ft
	283 337 Ft



	NEW!
	CSAMI702BT
	SAMI-702BT
	Installation audio mixer in standard rack format, featuring 6 MIC/LINE ST inputs, 1 BT input, 1 main mix balanced output and one AUX/REC additional output. It includes a 3 band tone control section, Talkover (priority) function assignable to each MIC/LINE input over the mix bus, 18V phantom available for all mic inputs, ST/MONO mix switch and MUTE port for external dry contact triggering. Dimensions
482.6 x 44(1RU) x 120 mm. Weight 1,8 kg
	600,99 €
	763,25 €
	243 400 Ft
	309 118 Ft



	DIGITAL MATRIXES & PROCESSORS	

	DIGITAL MATRIXES	
Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	NEW!
	CVIVOX8
	VIVO-X8
	VIVO-X8 is an EclerPLEX Host with 8 analogue and 8 Dante™/AES67 audio input ports, 8 analogue and 8 Dante/AES67 audio output ports, scalable thanks to two X-link ports. A BIO-X8 expansion unit can be connected to each X-link port. VIVO-X8 as a Host in an EclerPLEX project, can contain multiple projects running simultaneously and serve user panels.
	2 607,65 €
	3 311,72 €
	1 056 100 Ft
	1 341 247 Ft




	NEW!
	CBIOX8
	BIO-X8
	BIO-X8 is an affordable expansion interface that can easily scale up an VIVO-X8 digital matrix, adding to its default size, 8 input and 8 output analogue audio ports, 8 GPI ports and 8 GPO ports. A maximum of 2 BIO-X8 units can be linked to the same VIVO-X8, reaching a maximum total of 24 analogue audio input ports, 24 analogue audio output ports, 24 GPIs and 24 GPOs control ports.
	1 303,46 €
	1 655,39 €
	527 900 Ft
	670 433 Ft


Ref.
Name
MIMO Series
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CMIMO88	MIMO88	8 balanced MIC/LINE inputs / 8 balanced outputs + 2 monitor outputs digital audio matrix, fully	2 784,20 €
programmable through EclerNet Manager and linkable to a second unit to become a 16x16 matrix. Includes 8 GPI and 8 GPO ports. DSP processing: Parametric EQ & filters for each channel, delays, compressor/limiter, paging, priority, automatic mix (MIMO Firmware) and remote control via UCP or WPNETTOUCH.Dimensions 482.6 x 44 x 266.5 mm. Weight 3.5 kg
	3 535,93 €
	1 127 600 Ft
	1 432 052 Ft



	CMIMO88SG	MIMO88SG	8 balanced MIC/LINE inputs / 8 balanced outputs digital audio matrix, fully programmable through	1 804,94 €
EclerNet Manager. Includes 8 GPI ports. DSP processing: Parametric EQ & filters for each channel, delays, compressor/limiter, paging, priority, automatic mix (MIMO Firmware) and remote control via UCP or WPNETTOUCH. Dimensions 482.6 x 44 x 266.5 mm. Weight 3.5 kg
	2 292,27 €
	731 000 Ft
	928 370 Ft



	CMIMO1212SG	MIMO1212SG	12 balanced MIC/LINE inputs / 12 balanced outputs digital audio matrix, fully programmable through	2 077,78 €
EclerNet Manager. Includes 12 GPI ports. DSP processing: Parametric EQ & filters for each channel, delays, compressor/limiter, paging, priority, automatic mix (MIMO Firmware) and remote control via UCP or WPNETTOUCH. Dimensions 1RU x 266,5mm depth. Weight 3,5 kg
	2 638,78 €
	841 500 Ft
	1 068 705 Ft



	CMIMO4040CDN	MIMO4040CDN	Digital matrix with native processing of 40 inputs and 40 outputs (8 analogue inputs, 8 analogue	4 145,43 €
outputs, 32 Dante™ inputs and 32 Dante™ outputs). MIMO4040CDN comes with a CONFERENCE tailored firmware, including Automixer, Feedback Killer and Acoustic Echo Cancelling functions. It features accessories from WPNET Series connected by Ethernet. MIMO4040CDN is also capable of executing EclerNet projects thanks to its processor acting as a UCP server. Dimensions 482,6x44x266,5mm. Weight 3.25 kg
	5 264,70 €
	1 678 900 Ft
	2 132 203 Ft



	CM40AEC2EXP	M40AEC2EXP	Expansion license +2 AEC processing channels for MIMO4040CDN	112,59 €
*up to 8 AEC channels max. available in MIMO4040CDN
	142,99 €
	45 600 Ft
	57 912 Ft



	CM40AEC4EXP	M40AEC4EXP	Expansion license +4 AEC processing channels for MIMO4040CDN	225,93 €
*up to 8 AEC channels max. available in MIMO4040CDN
	286,93 €
	91 500 Ft
	116 205 Ft



	CM40AEC6EXP	M40AEC6EXP	Expansion license +6 AEC processing channels for MIMO4040CDN	339,26 €
*up to 8 AEC channels max. available in MIMO4040CDN
	430,86 €
	137 400 Ft
	174 498 Ft



	CMIMO7272DN	MIMO7272DN	64x64 native processing digital matrix with 72 inputs and 72 outputs (8 analogue inputs, 8 analogue	4 145,43 €
outputs, 64 Dante™ inputs and 64 Dante™ outputs). Incorporating audio over IP technology, MIMO7272DN allows signal transmission using a Local Ethernet network. It features accessories from WPNET Series connected by Ethernet. MIMO7272DN is also capable of executing EclerNet projects thanks to its processor acting as a UCP server. Dimensions 482,6x44x266,5mm. Weight 3.25 kg
	5 264,70 €
	1 678 900 Ft
	2 132 203 Ft


Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CDAM614C	DAM614	Fully programmable audio digital mixer. It includes 6 audio inputs (2x LINE ST + 4x LINE/MIC being	949,14 €
possible to use them independently (mono) or as stereo-coupled inputs) and 4 audio outputs (can be used as mono or stereo zones). Phantom power, front panel inputs and outputs level controls, DSP processing, RS-232 connectivity (compatible with EclerCOMM/CA-NET) and 4 REMOTE control ports (0- 10VDC). Dimensions 482.6 x 44(1RU) x 120 mm. Weight 2.00 kg
	1 205,40 €
	384 400 Ft
	488 188 Ft


DIGITAL ZONERS
Ref.
Name
HUB Series
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF



	CHUB1408	HUB1408	HUB1408 is a digital audio zoner with a global size of 14 input and 8 output analogue channels.	1 226,17 €
Available inputs are 4 MIC/LINE and 2 ST LINE local inputs, and 8 REMOTE LINE inputs. Available DSP: frequency shifter, link stereo, delay, crossover filters, graphic EQ, compressor/limiter and much more. Ecler pilot application, compatible with Android and iOS: control graphic panels set to user requirements. HxWxD: 88 (2RU) x 482,6 x 200mm. Weight 3,7 kg
	1 557,24 €
	496 600 Ft
	630 682 Ft



	CHUB1616	HUB1616	HUB1616 is a digital audio zoner with a global size of 16 input and 16 output analogue channels. The	1 651,36 €
input channels are: 4 channels for MIC/MONO LINE, 4 channels for ST LINE and 8 channels for MONO LINE received on the unit’s REMOTE ports, from wall panels eMCONTROL1. Available DSP: frequency shifter, link stereo, delay, crossover filters, graphic EQ, compressor/limiter and much more. Ecler pilot application, compatible with Android and iOS: control graphic panels set to user requirements. HxWxD: 88 (2RU) x 482,6 x 200mm. Weight 3,7 kg
	2 097,22 €
	668 800 Ft
	849 376 Ft





DANTE INTERFACES
Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF




	NEW!
	CBOB04
	BOB-04
	4 LINE outputs Dante™ Break Out Box. It allows taking up to 4 Dante™ channels from the Ethernet network and converting them to 4 analogue audio LINE level signals. PoE (Power over Ethernet) DC supply directly from PoE ready Ethernet switches (external AC power supply available as an optional accessory).
	500,74 €
	635,94 €
	202 800 Ft
	257 556 Ft



	NEW!
	CBOB22
	BOB-22
	2x MIC/LINE inputs and 2 LINE outputs Dante Break Out Box. It allows taking up to 2 Dante™ channels from the Ethernet network and converting them to 2 analogue audio
LINE level signals. It also allows taking up to 2 MIC/LINE analogue audio signals, convert them to 2 Dante™ channels and sent them to the Ethernet network. PoE (Power over Ethernet) DC supply directly from PoE ready Ethernet switches (external AC power supply available as an optional accessory).
	600,99 €
	763,25 €
	243 400 Ft
	309 118 Ft



	CDN44BOBC	DN44BOB	4 inputs/4 outputs DANTE (Audio Over IP) Break Out Box. It allows to convert 4 analogue audio signals	1 228,15 €
into 4 DANTE channels and send them into an Ethernet LAN, as well as to take 4 DANTE channels from the Ethernet network and convert them to analogue audio signals. It includes 4 GPI (0-10VDC) and 4 GPO control ports (NO/NC relays). Can be used together with EclerNet DANTE ready products or as a stand-alone DANTE interface. PUM3 included: rack-mount accessory to mount 2 halfwidth RU devices in 1 standard width RU space.
Dimensions 241 x 44(1RU) x 152 mm. Weight 1.1 kg
	1 559,75 €
	497 400 Ft
	631 698 Ft


LOUDSPEAKERS PROCESSORS
Ref.
Name
ALMA SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF



	CALMA24	ALMA24	Digital loudspeaker manager including 2 audio inputs and 4 audio outputs (all balanced), USB interface	646,17 €
and 2 volume remote control ports (0-10VDC). Includes DSP processor 24bits/48kHz, parametric EQ, 3 crossover types, 20 user presets and password protection.
ALMA24 is a 1RU stand-alone processor and EclerCOMM Manager compatibility. Dimensions 482.6 x 44 x 120 mm. Weight 1.75 kg
	820,64 €
	261 700 Ft
	332 359 Ft



	CALMA26	ALMA26	Digital loudspeaker manager including 2 audio inputs and 6 audio outputs (all balanced), USB interface	881,98 €
and 2 volume remote control ports (0-10VDC). Includes DSP processor 24bits/48kHz, parametric EQ, 3 crossover types, 20 user presets and password protection.
ALMA24 is a 1RU stand-alone processor and EclerCOMM Manager compatibility. Dimensions 482.6 x 44 x 120 mm. Peso 1.75 kg
	1 120,11 €
	357 200 Ft
	453 644 Ft



	AMPLIFIERS
	

	
	
	
	
	

	NETWORKABLE AMPLIFIERS
	
	
	
	

	
	
	
	
	

	Ref.	Name	VIDA SERIES
	Nettó lista ár EUR
	Bruttó lista ár EUR
	Nettó lista ár HUF
	Bruttó lista ár HUF



	CVIDA16Q	VIDA-16Q	1600W digital amplifier, with 4 amplified outputs that can be independently configured in high	2 720,00 €
(100/70V) or low (8/4/2ohm) impedance. The VersaPower technology, developed by Ecler, allows an asymmetrical power distribution. Max output power @ 2Ω/4Ω/8Ω or @70/100V - Single channel is 1600W. Audio player - with microSD slot for local audio files – as well as signal generator, plus 2 auxiliary line outputs and 4 Dante digital outputs. Internal matrix and signal processing. Remote control user application for iOS/Android/Web. Control and scheduled events for automation. Ultra low power consumption mode. Dimensions 482,6x88(2RU)x410 mm / 19"x3.46"x16.14". Weight 9,3 kg. /
20.5 lb.
	3 454,40 €
	1 101 600 Ft
	1 399 032 Ft



	CVIDA24Q	VIDA-24Q	2400W digital amplifier, with 4 amplified outputs that can be independently configured in high	3 081,98 €
(100/70V) or low (8/4/2ohm) impedance. Max output power @ 2Ω/4Ω/8Ω or @70/100V – 4x600W /4 Ω symetrical power distribution. The VersaPower technology, developed by Ecler, allows an asymmetrical power distribution with a max output power @ 4Ω or 100V – into one single channel 2400W. Audio player - with microSD slot for local audio files – as well as signal generator, plus 2 auxiliary line outputs and 4 Dante digital outputs. Internal matrix and signal processing. Remote control user application for iOS/Android/Web. Control and scheduled events for automation. Ultra low power consumption mode. Dimensions 482,6x88(2RU)x410 mm / 19"x3.46"x16.14". Weight 9,3 kg. /
20.5 lb.
	3 914,11 €
	1 248 200 Ft
	1 585 214 Ft



	CVIDA48Q	VIDA-48Q	4800W digital amplifier, with 4 amplified outputs that can be independently configured in high	3 697,04 €
(100/70V) or low (8/4/2ohm) impedance. The VersaPower technology, developed by Ecler, allows an asymmetrical power distribution. Max output power @ 2Ω/4Ω/8Ω or @70/100V - Single channel is 2600W. Audio player - with microSD slot for local audio files – as well as signal generator, plus 2 auxiliary line outputs and 4 Dante digital outputs. Internal matrix and signal processing. Remote control user application for iOS/Android/Web. Control and scheduled events for automation. Ultra low power consumption mode. Dimensions 482,6x88(2RU)x410 mm / 19"x3.46"x16.14". Weight 9,3 kg. /
20.5 lb.
	4 695,24 €
	1 497 300 Ft
	1 901 571 Ft


Ref.
Name
HALO SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	NEW!
	CHALO2B300
	HALO-2B300
	2x300W amplifier, with 2 powered outputs usable as Low and High Impedance. Bridge between outputs should be used in High impedance or to double the power in Low Impedance. The built-in web interface (similar to VIDA Series) allows easy programming and control of basic or advanced functions, thanks to different access levels. All models include a single Ethernet interface for setup, control and Dante™/AES67 protocol. Flexible end user control through customizable user panels, accessible via web GUI or mobile application.
	TBC
	TBC
	TBC
	TBC




	NEW!
	CHALO4B150
	HALO-4B150
	4x150W amplifier, with 2 powered outputs usable as Low and High Impedance. Bridge between outputs should be used in High impedance or to double the power in Low Impedance. The built-in web interface (similar to VIDA Series) allows easy programming and control of basic or advanced functions, thanks to different access levels. All models include a single Ethernet interface for setup, control and Dante™/AES67 protocol. Flexible end user control through customizable user panels, accessible via web GUI or mobile application.
	TBC
	TBC
	TBC
	TBC



	NEW!
	CHALO4B300
	HALO-4B300
	4x300W amplifier, with 2 powered outputs usable as Low and High Impedance. Bridge between outputs should be used in High impedance or to double the power in Low Impedance. The built-in web interface (similar to VIDA Series) allows easy programming and control of basic or advanced functions, thanks to different access levels. All models include a single Ethernet interface for setup, control and Dante™/AES67 protocol. Flexible end user control through customizable user panels, accessible via web GUI or mobile application.
	TBC
	TBC
	TBC
	TBC


Ref.
Name
HADA SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CHADA4B150	HADA-4B150	HADA-4B150 is a 4x125W digital amplifier that supports low and high impedance loads. The internal	1 264,20 €
DSP, through the HADA DSP Manager software, allows tailoring the input and output signal through parametric EQs, multi-band compressors, limiters, and delays and each configuration can be saved as a preset.. Dimensions 482.6 x 88 x 281,5 mm / 19 x 3.46 x 11.08 in. Weight 4.7 Kg / 10.36 lbs
	1 605,53 €
	512 000 Ft
	650 240 Ft



	CHADA4B250	HADA-4B250	HADA-4B250 is a 4x250W digital amplifier that supports low and high impedance loads. The internal	1 366,67 €
DSP, through the HADA DSP Manager software, allows tailoring the input and output signal through parametric EQs, multi-band compressors, limiters, and delays and each configuration can be saved as a preset.. Dimensions 482.6 x 88 x 281,5 mm / 19 x 3.46 x 11.08 in. Weight 5.0 Kg / 11.02 lb
	1 735,67 €
	553 500 Ft
	702 945 Ft



	CHADA4B400	HADA-4B400	HADA-4B400 is a 4x400W digital amplifier that supports low and high impedance loads. The internal	1 489,88 €
DSP, through the HADA DSP Manager software, allows tailoring the input and output signal through parametric EQs, multi-band compressors, limiters, and delays and each configuration can be saved as a preset.. Dimensions 482.6 x 88 x 281,5 mm / 19 x 3.46 x 11.08 in. Weight 5.4 Kg / 11.91 lb
	1 892,14 €
	603 400 Ft
	766 318 Ft



	CHADA4B500	HADA-4B500	HADA-4B500 is a 4x500W digital amplifier that supports low and high impedance loads. The internal	1 593,33 €
DSP, through the HADA DSP Manager software, allows tailoring the input and output signal through parametric EQs, multi-band compressors, limiters, and delays and each configuration can be saved as a preset.. Dimensions 482.6 x 88 x 281,5 mm / 19 x 3.46 x 11.08 in. 5.6 Kg / 12.35 lb
	2 023,53 €
	645 300 Ft
	819 531 Ft



	CHADA4B750	HADA-4B750	HADA-4B750 is a 4x750W digital amplifier that supports low and high impedance loads. The internal	1 952,35 €
DSP, through the HADA DSP Manager software, allows tailoring the input and output signal through parametric EQs, multi-band compressors, limiters, and delays and each configuration can be saved as a preset.. Dimensions 482.6 x 88 x 281,5 mm / 19 x 3.46 x 11.08 in. Weight 6.0 Kg / 13.22 lb
	2 479,48 €
	790 700 Ft
	1 004 189 Ft


Ref.
Name
NXA SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	EOL
	CNXA480
	NXA 4-80
	4 in/4 out self-powered digital manager that stays halfway between a digital matrix and a class D multichannel amplifier (4 x 85W @ 4Ω RMS). Includes a powerful DSP processor, auto stand-by function, convection cooling, health self-test mode function and 4 GPI ports. Compatible with EclerNet Manager platform and UCP remote control system. Dimensions 482.6 x 88 x 373 mm. Weight 9.2 kg
	1 597,28 €
	2 028,55 €
	646 900 Ft
	821 563 Ft



	EOL
	CNXA4200
	NXA 4-200
	4 in /4 out self-powered digital manager that stays halfway between a digital matrix and a class D multichannel amplifier (4 x 202W @ 4Ω RMS). Includes a powerful DSP processor, auto stand-by function, convection cooling, health self-test mode function and 4 GPI ports. Compatible with EclerNet Manager platform and UCP remote control system. Dimensions 482.6 x 88(2RU) x 373 mm. Weight
12.6 kg
	2 224,44 €
	2 825,04 €
	900 900 Ft
	1 144 143 Ft



	EOL
	CNXA4400
	NXA 4-400
	4 in /4 out self-powered digital manager that stays halfway between a digital matrix and a class D multichannel amplifier (4 x 416W @ 4Ω RMS). Includes a powerful DSP processor, auto stand-by function, convection cooling, health self-test mode function and 4 GPI ports. Compatible with EclerNet Manager platform and UCP remote control system. Dimensions 482. 6x 88(2RU) x 373 mm. Weight
16.0 kg
	3 086,17 €
	3 919,44 €
	1 249 900 Ft
	1 587 373 Ft



	COMMERCIAL AMPLIFIERS	
Ref.
Name
AURA SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CAURA2H150	AURA-2H150	Stereo amplifier with 2 x 150 WRMS @ 70/100V (high impedance) powered outputs. Iincludes the	770,62 €
option to link channels to the first input via a rear panel selector, as well as auto stand-by, overload and thermal protection, PFC, and an anti-clipping system. The front panel volume knobs can be locked using rear panel switches. Dimensions 440 x 44(1RU) x 221mm. Weight 6.05 kg
	978,68 €
	312 100 Ft
	396 367 Ft



	CAURA4H150	AURA-4H150	Multichannel amplifier with 4 x 150 WRMS @ 70/100V (high impedance) powered outputs. Includes	1 129,88 €
the option to link channels to the first input via a rear panel selector, as well as auto stand-by, overload and thermal protection, PFC, and an anti-clipping system. The front panel volume knobs can be locked using rear panel switches. Dimensions 440 x 44(1RU) x 341mm. Weight 10.5 kg
	1 434,94 €
	457 600 Ft
	581 152 Ft



	CAURA2L150	AURA-2L150	Stereo 2x150 WRMS @ 4 Ω, high efficiency amplifier. Includes the option to link channels to the first	564,94 €
input via a rear panel selector, as well as auto stand-by, overload and thermal protection, PFC, and an anti-clipping system. The front panel volume knobs can be locked using rear panel switches.
Dimensions 440 x 44(1RU) x 161 mm. Weight 2.60 kg
	717,47 €
	228 800 Ft
	290 576 Ft



	CAURA4L150	AURA-4L150	4x150 WRMS @ 4 Ω, high efficiency multichannel amplifier. Includes the option to link channels to the	821,73 €
first input via a rear panel selector, as well as auto stand-by, overload and thermal protection, PFC, and an anti-clipping system. The front panel volume knobs can be locked using rear panel switches.
Dimensions 482.6 x 44(1RU) x 221 mm. Weight 3.60 kg
	1 043,60 €
	332 800 Ft
	422 656 Ft



	CAURA8L150	AURA-8L150	8x150 WRMS @ 4 Ω, high efficiency multichannel amplifier. Includes the option to link channels to the	1 540,99 €
first input via a rear panel selector, as well as auto stand-by, overload and thermal protection, PFC, and an anti-clipping system. The front panel volume knobs can be locked using rear panel switches.
Dimensions 482.6 x 44(1RU) x 341 mm. Weight 6 kg
	1 957,05 €
	624 100 Ft
	792 607 Ft



	NEW!
	CAURA2B600
	AURA-2B600
	2x600WRMS @ 4Ω offering compatibility with both LoZ (2/4/8Ω) and HiZ (70/100V) configurations and supporting dual or bridge mode (@4/8Ω). AURA Series also includes the option to link channels to the first input via a rear panel selector, as well as auto stand-by, overload and thermal protection, PFC, and an anti-clipping system. The front panel volume knobs can be locked using rear panel switches.
	801,73 €
	1 018,20 €
	324 700 Ft
	412 369 Ft



	NEW!
	CAURA2B900
	AURA-2B900
	2x900WRMS @ 4Ω offering compatibility with both LoZ (2/4/8Ω) and HiZ (70/100V) configurations and supporting dual or bridge mode (@4/8Ω). AURA Series also includes the option to link channels to the first input via a rear panel selector, as well as auto stand-by, overload and thermal protection, PFC, and an anti-clipping system. The front panel volume knobs can be locked using rear panel switches.
	1 002,47 €
	1 273,14 €
	406 000 Ft
	515 620 Ft



	NEW!
	CAURA4B600
	AURA-4B600
	4x600WRMS @ 4Ω offering compatibility with both LoZ (2/4/8Ω) and HiZ (70/100V) configurations and supporting dual or bridge mode (@4/8Ω). AURA Series also includes the option to link channels to the first input via a rear panel selector, as well as auto stand-by, overload and thermal protection, PFC, and an anti-clipping system. The front panel volume knobs can be locked using rear panel switches.
	1 303,46 €
	1 655,39 €
	527 900 Ft
	670 433 Ft



	NEW!
	CAURA4B900
	AURA-4B900
	4x900WRMS @ 4Ω offering compatibility with both LoZ (2/4/8Ω) and HiZ (70/100V) configurations and supporting dual or bridge mode (@4/8Ω). AURA Series also includes the option to link channels to the first input via a rear panel selector, as well as auto stand-by, overload and thermal protection, PFC, and an anti-clipping system. The front panel volume knobs can be locked using rear panel switches.
	1 554,07 €
	1 973,67 €
	629 400 Ft
	799 338 Ft


Ref.
Name
eLPA SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CELPA2350	eLPA2-350	Stereo amplifier delivering 2 x 345 WRMS @ 4Ω. Have 2 XLR balanced inputs, 2 Speakon® and terminal	662,22 €
type connection outputs. Ultra light and versatile format. Built in crossover (150Hz), permanently activated anti-clip circuit and efficient progressive ventilation system.2 Bridged Channels @ 8 Ω 560 WRMS. Dimensions 482.6 x 88(2RU) x 266 mm. Weight 5.50 kg
	841,02 €
	268 200 Ft
	340 614 Ft



	CELPA2650	eLPA2-650	Stereo amplifier delivering 2 x 630 WRMS @ 4Ω. Have 2 XLR balanced inputs, 2 Speakon® and terminal	849,88 €
type connection outputs. Ultra light and versatile format. Permanently activated anti-clip circuit and efficient progressive ventilation system. 2 Bridged Channels @ 8 Ω 1220 WRMS. Dimensions 482.6 x 88(2RU) x 266 mm / 6.00kg
	1 079,34 €
	344 200 Ft
	437 134 Ft



	CELPA2950	eLPA2-950	Stereo amplifier delivering 2 x 950 WRMS @ 4Ω. Have 2 XLR balanced inputs, 2 Speakon® and terminal	999,26 €
type connection outputs. Ultra light and versatile format. Permanently activated anti-clip circuit and efficient progressive ventilation system. 2 Bridged Channels @ 8 Ω 1840 WRMS. Dimensions 482,6 x 88(2RU)x 266 mm. Weight 6,15 kg
	1 269,06 €
	404 700 Ft
	513 969 Ft



	CELPA21400	eLPA2-1400	Stereo amplifier delivering 2 x 1400 WRMS @ 4Ω. Have 2 XLR balanced inputs, 2 Speakon® and	1 129,88 €
terminal type connection outputs. Ultra light and versatile format. Permanently activated anti-clip circuit and efficient progressive ventilation system. 2 Bridged Channels @ 8 Ω 2600 WRMS. Dimensions 482,6 x 88(2RU) x 304 mm. Weight 6,35 kg
	1 434,94 €
	457 600 Ft
	581 152 Ft


Ref.
Name
eGPA SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CEGPA2300	eGPA2-300	Stereo, 2x310 WRMS @ 4 Ω, high efficiency stereo amplifier (class D). Auto stand-by function, fanless	718,52 €
design 100% silent. 2 Bridged Channels @ 8Ω 600 WRMS. Dimensions 440 x 44(1RU) x 221 mm. Weight
3.40 kg
	912,52 €
	291 000 Ft
	369 570 Ft



Ref.
Name
GPA SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CGPA2400ES	GPA2-400ES	Stereo amplifier delivering 2 x 350 WRMS @ 4 Ω. True green profile: high efficiency, auto stand-by	976,30 €
function, 100% silent fanless design, Energy Star certified. 2 remote volume control ports and bridge mode 2 channels @ 8Ω 700 WRMS. Dimensions 482.6 x 88(2RU) x 373 mm. Weight 10.8 kg
	1 239,90 €
	395 400 Ft
	502 158 Ft



	CGPA2800	GPA2-800	Stereo amplifier delivering 2 x 720 WRMS @ 4 Ω, and ready to drive 1000 WRMS @ 2Ω loudspeaker	1 335,56 €
loads (4 x 8 Ω loudspeakers in parallel, per channel). True green profile: high efficiency, auto stand-by function, 100% silent fanless design. 2 remote volume control ports and bridge mode 2 Channels @ 8Ω 1150 WRMS. Dimensions 482.6 x 88(2RU) x 373 mm. Weight 10.8 kg
	1 696,16 €
	540 900 Ft
	686 943 Ft


Ref.
Name
eHSA SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CEHSA460	eHSA4-60	Multichannel amplifier Class D with 4x60 WRMS @ 70/100V (high impedance) powered outputs, and	770,62 €
low impedance output. Its noiseless convection cooling, and its auto stand-by function provide this amplifier with a true green profile. Include link channel buttons, that allows to replicate the input channel signal in the adjacent one. Dimensions 482,6 x 44(1RU) x 280mm. Weight 7,8 kg
	978,68 €
	312 100 Ft
	396 367 Ft



	CHSA2400ES	HSA2-400ES	Stereo amplifier with low and high impedance powered outputs (2x400 WRMS). Includes 2 balanced	1 243,21 €
inputs (XLR and Euroblock), 2 remote volume ports and Euroblock outputs. True green profile( Energy Star® Certification): auto stand-by function and noiseless convection cooling. Dimensions 482.6 x 88(2RU) x 373 mm. Weight 16.4 kg
	1 578,88 €
	503 500 Ft
	639 445 Ft


MIXING AMPLIFIERS
Ref.
Name
eHMA SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF



	CEHMA60C	eHMA60	Self-powered audio mixer including 1 MIC input and two MIC/LINE ST inputs. It features a 60W	369,38 €
powered output that supports both low (4 Ω) and high impedance (70/100V) loudspeaker lines. It also includes an audio priority system, phantom power, 2 band tone control, auto stand-by mode, MUTE port and universal power supply unit (24 VDC IN).Dimensions 200x44x150 mm. Weight 1.9kg.
1UHRMKIT Rack Mount Kit included.
	469,12 €
	149 600 Ft
	189 992 Ft



	CEHMA120C	eHMA120	Stereo, Self-powered audio mixer including 3x MIC/LINE ST and 1x LINE ST input. It features a 95W	545,93 €
powered mono output that supports both low (4Ω) and high impedance (70/100V) loudspeaker lines, with 2-ZONE ON/OFF switches. Includes audio priority system, pager (1 zone), phantom, 2 band tone control, auto stand-by, MUTE port and universal power supply unit (compatible with 24 VDC IN).
Dimensions 435x44x120 mm. Weight 2.9kg 1UHRMKIT Rack Mount Kit included
	693,33 €
	221 100 Ft
	280 797 Ft



	CEHMA250	eHMA250	Self-powered audio mixer including 2 MIC, 2 MIC/LINE ST and 2 LINE ST inputs. It features a 250W	856,79 €
powered mono output that supports both low (4 and 8Ω) and high impedance (50/70/100V) loudspeaker lines, with 4-ZONE ON/OFF switches. Includes an audio priority system, Pager (1 zone), phantom power, remote control port (WPm), AUX/REC output, 2 band tone control, auto stand-by mode and MUTE port. Dimensions 435x220x44mm / 17,1”x8,7”x1,7”mm. Weight 3kg / 6.6lb.
	1 088,12 €
	347 000 Ft
	440 690 Ft


Ref.	Name	HMA SERIES	RRP €	RRP €	RRP €	RRP €


	CHMA120	HMA120	Self-powered mixer including an integrated media player (USB,SD) and 5 external audio inputs: 3 x LINE	646,17 €
ST, 1 MIC/LINE and 1 MIC. It features a 120W powered output that supports both low (4Ω) and high impedance (70/100V) loudspeaker lines. It also includes a 2 level priority system, auto stand-by mode, 2 band control tone, AUX OUT and a remote control port WPm series compatible. Dimensions 210 x 88 x 230 mm. Weight 5.95 kg Compatible with the 2UHRMKIT Rack Mount Kit.
	820,64 €
	261 700 Ft
	332 359 Ft


ULTRA COMPACT AMPLIFIERS
Ref.
Name
CA SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF



	CCA40	CA40	2 x 20 WRMS @ 4Ω stereo compact amplifier with a balanced MIC input (includes phantom power,	352,35 €
Talkover and noise gate) and 2 LINE inputs. 3 output modes (STEREO, PARALLEL and BRIDGE) and AUX output. 2 band control tone, IR remote control included, serial RS-232 port (EclerCOMM and CA-NET compatible) and 0-10 VDC remote port for WPm wall panel series (volume and source selection). Auto- standby function and MUTE port. Dimensions 155 x 155 x 45 mm. Weight 0.65 kg
	447,48 €
	142 700 Ft
	181 229 Ft



	CCA120C	CA120	2 x 60 WRMS @ 4Ω stereo compact amplifier with a MIC/LINE input (includes phantom power,	516,79 €
Talkover and noise gate) and 2 LINE inputs. AUX output. Control features: 2 band control tone, IR remote control included, serial RS-232 port (EclerCOMM and CA-NET compatible) and 0-10 VDC remote port for WPm wall panel series (volume and source selection). Auto-standby function and MUTE port. Dimensions 160 x 210 x 48 mm. Weight 0.95 kg
	656,32 €
	209 300 Ft
	265 811 Ft



	CCA120HZC	CA120HZ	High impedance version of the CA120, delivering 120W @ 70/100V line level, with a MIC/LINE input	557,04 €
(includes phantom power, Talkover and noise gate) and 2 LINE inputs. AUX output. Control features: 2 band control tone, IR remote control included, serial RS-232 port (EclerCOMM and CA-NET compatible) and 0-10 VDC remote port for WPm wall panel series (volume and source selection). Auto-standby function and MUTE port. Dimensions 160 x 325 x 48 mm. Weight 2.92 kg
	707,44 €
	225 600 Ft
	286 512 Ft





Ref.
Name
eCA SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF

	CECA120C	eCA120	2 x 60 WRMS @ 4 Ω stereo micro-amplifier, in a very compact format and a light and silent (fanless)	418,52 €
design. It features 1 LINE ST input (RCA/Euroblock), AUTO STANDBY function and volume remote control, compatible with Ecler WPmVOL and WPmVOL-SR wall panels (0-10 VDC). Auto-standby function. External, universal and CE/UL/CCC certified power supply. Dimensions: 190 x 48 x 90mm. Weight 600 g.
	531,52 €
	169 500 Ft
	215 265 Ft



	CECA120HZC	eCA120HZ	Mono micro-amplifier delivering 1 x 120 WRMS @ 70V / 100 V line level (high impedance), built in a	473,58 €
very compact format and a light and silent (fanless) design. It features 1 LINE ST input (RCA/Euroblock), AUTO STANDBY function and volume remote control, compatible with WPmVOL and WPmVOL-SR wall panels (0-10 VDC). Auto-standby function.
External, universal and CE/UL/CCC certified power supply. Dimensions: 190 x 48 x 190mm. Weight 2.3 kg
	601,45 €
	191 800 Ft
	243 586 Ft



	LOUDSPEAKERS
	

	
	
	
	
	

	IN-CEILING LOUDSPEAKERS
	
	
	
	

	
	
	
	
	

	Ref.	Name
	Nettó lista ár EUR
	Bruttó lista ár EUR
	Nettó lista ár HUF
	Bruttó lista ár HUF



	CIW103	IW103	3" in-ceiling / in-wall installation loudspeaker featuring a rectangular and discreet design, and including	81,48 €
a high impedance transformer unit with 15 and 30 W power selections @ 100V line level. Dimensions 110 x 165 x 80 mm. Weight 900g. Delivered by master carton of 8 units. Price per unit.
	103,48 €
	33 000 Ft
	41 910 Ft


Ref.
Name
eIC SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CEIC51FM	eIC51FM	Fast installation in-ceiling loudspeaker. It features a 4,5" woofer, 6 WRMS @ 8 Ω nominal power and	23,21 €
70/100V line transformer with 3 and 6 W power selections. Internal diameter 150 mm. External diameter 160mm. Required depth 54mm. Weight 500g. Price per unit.
	29,48 €
	9 400 Ft
	11 938 Ft



	CEIC52	eIC52	2-way cost-effective in-ceiling loudspeaker with a great sound performance. It features a 5,25" woofer	43,21 €
and a 0,75" tweeter, 20 WRMS @ 8 Ω nominal power and 100V line transformer with 3 and 6 W power selections. Internal diameter 164mm. External diameter 202mm. Required depth: 65mm. Weight 1.0 kg Delivered by master carton of 8 units. Price per unit.
	54,88 €
	17 500 Ft
	22 225 Ft



	CEIC52MS	eIC52MS	2-way in-ceiling loudspeaker suitable for installations exposed to extreme humidity and/or	64,44 €
temperature. It features 1x5" woofer and 1x1" tweeter with a global power admission of 20 WRMS @ 8Ω. Internal diameter 120mm. External diameter 165mm. Required depth 79mm. Weight 700g.
Delivered by units. Price per unit.
	81,84 €
	26 100 Ft
	33 147 Ft


Ref.
Name
IC SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CIC3BK	IC3	1-way loudspeaker is the perfect option for 70/100 V (0.75/1.5/3/6 W) and low impedance sound	50,37 €
solutions. It mounts a 3” woofer in a discreet design. Cutout size 90mm. Internal diameter 88mm. External diameter 105mm. Required depth 90mm. Weight 500g. Black colour. Delivered by master carton of 2 units. Price per unit.
	63,97 €
	20 400 Ft
	25 908 Ft



	CIC3WH	IC3	1-way loudspeaker is the perfect option for 70/100 V (0.75/1.5/3/6 W) and low impedance sound	50,37 €
solutions. It mounts a 3” woofer in a discreet design. Cutout size 90mm. Internal diameter 88mm. External diameter 105mm. Required depth 90mm. White colour. Weight 500g. Delivered by master carton of 2 units. Price per unit.
	63,97 €
	20 400 Ft
	25 908 Ft



	CIC6BK	IC6BK	2-way loudspeaker is the perfect option for 70/100 V (2.5/5/7.5/15 W) and low impedance sound	69,38 €
solutions (40 WRMS @8Ω). It mounts a 6” woofer and a 1" tweeter in a discreet design. Cutout size 180mm. Internal diameter 178mm. External diameter 204mm. Required depth 73mm. Weight 1,52kg Delivered by master carton of 2 units. Price per unit. Black colour.
	88,12 €
	28 100 Ft
	35 687 Ft



	CIC6	IC6	2-way loudspeaker is the perfect option for 70/100 V (2.5/5/7.5/15 W) and low impedance sound	69,38 €
solutions (40 WRMS @8Ω). It mounts a 6” woofer and a 1" tweeter in a discreet design. Cutout size 180mm. Internal diameter 178mm. External diameter 204mm. Required depth 73mm. Weight 1,52kg Delivered by master carton of 2 units. Price per unit. White colour.
	88,12 €
	28 100 Ft
	35 687 Ft



	CIC8	IC8	2-way loudspeaker is the perfect option for 70/100 V (5/7.5/15/30 W) and low impedance sound	97,53 €
solutions (60 WRMS @8Ω). It mounts an 8” woofer and a 1" tweeter in a discreet design. Cutout size 222mm. Internal diameter 220mm. External diameter 245mm. Required depth 91mm. Weight 2,3kg Delivered by master carton of 2 units. Price per unit. White colour.
	123,86 €
	39 500 Ft
	50 165 Ft




	NEW!
	CIC6IBK

[image: ]

[image: ]
	IC6i
	2-way loudspeaker is the perfect option for 70/100 V (2.5/5/7.5/15 W) and low impedance sound solutions (40 WRMS @8Ω). It mounts a 6” woofer and a 1" tweeter in a discreet design. Cutout size 180mm. Internal diameter 178mm. External diameter 204mm. Required depth 73mm. Magnetic Grille. Weight 1,52kg Delivered by master carton of 2 units. Price per unit. Black colour.
	69,38 €
	88,12 €
	28 100 Ft
	35 687 Ft



	NEW!
	CIC6IWH

[image: ]
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	IC6i
	2-way loudspeaker is the perfect option for 70/100 V (2.5/5/7.5/15 W) and low impedance sound solutions (40 WRMS @8Ω). It mounts a 6” woofer and a 1" tweeter in a discreet design. Cutout size 180mm. Internal diameter 178mm. External diameter 204mm. Required depth 73mm. Magnetic Grille. Weight 1,52kg Delivered by master carton of 2 units. Price per unit. White colour.
	69,38 €
	88,12 €
	28 100 Ft
	35 687 Ft



	NEW!
	CIC8IWH
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	 IC8i
	2-way loudspeaker is the perfect option for 70/100 V (5/7.5/15/30 W) and low impedance sound solutions (60 WRMS @8Ω). It mounts an 8” woofer and a 1" tweeter in a discreet design. Cutout size 222mm. Internal diameter 220mm. External diameter 245mm. Required depth 91mm. Magnetic Grille. Weight 2,3kg. Delivered by master carton of 2 units. Price per unit. White colour.
	97,53 €
	123,86 €
	39 500 Ft
	50 165 Ft


Ref.
Name
VIC SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CVIC6	VIC6	2-way loudspeaker is the perfect option for 70/100 V (2,5/5/10/20/40 W) and low impedance sound	110,37 €
solutions (40 WRMS @8Ω). It mounts a 6,5” woofer and a 0,5" steerable tweeter in a discreet design. Dimensions (ØxD): 232x105mm. Weight 1,8kg.
Delivered by master carton of 2 units. Price per unit.
	140,17 €
	44 700 Ft
	56 769 Ft



	CVIC6X	VIC6X	2-way loudspeaker is the perfect option for 70/100 V (2,5/5/10/20/40 W) and low impedance sound	175,80 €
solutions (40 WRMS @8Ω). It mounts a 6,5” woofer and a 0,5" steerable tweeter in a discreet design. With plastic back can and tile bridge.
Dimensions (ØxD): 232x170mm. Weight 1,8kg. Delivered by master carton of 2 units. Price per unit.
	223,27 €
	71 200 Ft
	90 424 Ft



	CVIC8	VIC8	2-way loudspeaker is the perfect option for 70/100 V (3,75/7,5/15/30/60 W) and low impedance sound	140,49 €
solutions (60 WRMS @8Ω). It mounts an 8” woofer and a 0,5" steerable tweeter in a discreet design. Dimensions (ØxD): 282x115mm. Weight 2,3kg.
Delivered by master carton of 2 units. Price per unit.
	178,43 €
	56 900 Ft
	72 263 Ft



	CVIC8X	VIC8X	2-way loudspeaker is the perfect option for 70/100 V (3,75/7,5/15/30/60 W) and low impedance sound	249,88 €
solutions (60 WRMS @8Ω). It mounts an 8” woofer and a 0,5" steerable tweeter in a discreet design. With plastic back can and tile bridge.
Dimensions (ØxD): 282x200mm. Weight 3,1kg. Delivered by master carton of 2 units. Price per unit.
	317,34 €
	101 200 Ft
	128 524 Ft



	CVICSB81	VICSB8	Sub-woofer reinforcement loudspeaker is the perfect option for 70/100 V (3,75/7,5/15/30/60 W) and	237 €
low impedance sound solutions. It mounts an 8” providing 80 WRMS power in a discreet design.Dimensions (ØxD): 282x135mm. Weight 3,1kg.
Delivered by units. Price per unit.
	237 €
	101 200 Ft
	128 524 Ft



	CVICSB8X	VICSB8X	Sub-woofer reinforcement loudspeaker is the perfect option for 70/100 V (3,75/7,5/15/30/60 W) and	360,25 €
low impedance sound solutions. It mounts an 8” providing 80 WRMS power in a discreet design. With plastic back can and tile bridge.
Dimensions (ØxD): 282x200mm. Weight 3,9kg. Delivered by master carton of 2 units. Price per unit.
	457,51 €
	145 900 Ft
	185 293 Ft



	HIGH PERFORMANCE LOUDSPEAKERS	
Ref.
Name
MIA SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CMIA81BK	MIA-81	MIA-81 is a an elegant, unique a compact design column loudspeaker, built in a single aluminium piece	580,99 €
to avoid vibrations and mechanical stress. MIA-81 includes 8x1.5” drivers delivering 40WRMS and the possibility of working in 16 Ω or 64 Ω. IP44 rated. Includes FLATY bracket made out of stainless-steel that permits adjusting the height at any point of the length of the column. Black colour. Dimensions 58 x 448 x 67 mm / 2.28 x 17.64 x 2.64 in. (WxHxD). Weight 1.2 kg / 1.64 lb. Delivered by units. Price per unit.
	737,85 €
	235 300 Ft
	298 831 Ft



	CMIA81WH	MIA-81	MIA-81 is a an elegant, unique a compact design column loudspeaker, built in a single aluminium piece	580,99 €
to avoid vibrations and mechanical stress. MIA-81 includes 8x1.5” drivers delivering 40WRMS and the possibility of working in 16 Ω or 64 Ω. IP44 rated. Includes FLATY bracket made out of stainless-steel that permits adjusting the height at any point of the length of the column. White colour. Dimensions 58 x 448 x 67 mm / 2.28 x 17.64 x 2.64 in. (WxHxD). Weight 1.2 kg / 1.64 lb. Delivered by units. Price per unit.
	737,85 €
	235 300 Ft
	298 831 Ft




	CMIA82BK	MIA-82	MIA-82 is a an elegant, unique a compact design column loudspeaker, built in a single aluminium piece	767,65 €
to avoid vibrations and mechanical stress. MIA-82 includes 8x2.5” drivers delivering 150WRMS and the possibility of working in 16 Ω or 64 Ω. IP44 rated. Includes the versatile smart pan and tilt bracket HANDY made out of stainless-steel that permits adjusting the height at any point of the length of the column. Black colour. Dimensions 83 x 648 x 87 mm / 3.27 x 25.51 x 3.43 in. (WxHxD). Weight 2.65 kg /
5.84 lb. Delivered by units. Price per unit.
	974,92 €
	310 900 Ft
	394 843 Ft



	CMIA82WH	MIA-82	MIA-82 is a an elegant, unique a compact design column loudspeaker, built in a single aluminium piece	767,65 €
to avoid vibrations and mechanical stress. MIA-82 includes 8x2.5” drivers delivering 150WRMS and the possibility of working in 16 Ω or 64 Ω. IP44 rated. Includes the versatile smart pan and tilt bracket HANDY made out of stainless-steel that permits adjusting the height at any point of the length of the column. White colour. Dimensions 83 x 648 x 87 mm / 3.27 x 25.51 x 3.43 in. (WxHxD). Weight 2.65 kg
/ 5.84 lb. Delivered by units. Price per unit.
	974,92 €
	310 900 Ft
	394 843 Ft


Ref.
Name
NIMBO SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CNIMBO14WH	NIMBO-14	2-way passive loudspeaker for surface mounting (1x 4" woofers and 1" tweeter). 40 WRMS @ 8 ohm.	353,33 €
Suitable for outdoor applications, with a wide dispersion pattern and IP-44 rating. White color. Dimensions 250 x 148.7x 150 mm / 9.84 x 5.85 x 5.91 in. Weight 1.7 kg / 3.75 lb. Delivered by units. Price per unit.
	448,73 €
	143 100 Ft
	181 737 Ft



	CNIMBO14BK	NIMBO-14	2-way passive loudspeaker for surface mounting (1x 4" woofers and 1" tweeter). 40 WRMS @ 8 ohm.	353,33 €
Suitable for outdoor applications, with a wide dispersion pattern and IP-44 rating. Black color. Dimensions 250 x 148.7x 150 mm / 9.84 x 5.85 x 5.91 in. Weight 1.7 kg / 3.75 lb. Delivered by units. Price per unit.
	448,73 €
	143 100 Ft
	181 737 Ft



	CNIMBO14GD	NIMBO-14	2-way passive loudspeaker for surface mounting (1x 4" woofers and 1" tweeter). 40 WRMS @ 8 ohm.	353,33 €
Suitable for outdoor applications, with a wide dispersion pattern and IP-44 rating. Gold color. Dimensions 250 x 148.7x 150 mm / 9.84 x 5.85 x 5.91 in. Weight 1.7 kg / 3.75 lb. Delivered by units. Price per unit.
	448,73 €
	143 100 Ft
	181 737 Ft



	NEW!
	CNIMBO14TN
[image: ]

	NIMBO-14
	2-way passive loudspeaker for surface mounting (1x 4" woofers and 1" tweeter). 40 WRMS @ 8 ohm. Suitable for outdoor applications, with a wide dispersion pattern and IP-44 rating. Titanium color.
Dimensions 250 x 148.7x 150 mm / 9.84 x 5.85 x 5.91 in. Weight 1.7 kg / 3.75 lb. Delivered by units. Price per unit.
	353,33 €
	448,73 €
	143 100 Ft
	181 737 Ft



	CNIMBO14CR	NIMBO-14	NIMBO-14 cabinet RAL customization (black grill and bracket). MOQ: 8 units. Delivery time: 45 days.	405,43 €
Dimensions 250 x 148.7x 150 mm / 9.84 x 5.85 x 5.91 in. Weight 1.7 kg / 3.75 lb. Delivered by units. Price per unit.
	514,90 €
	164 200 Ft
	208 534 Ft



	CNIMBO24WH	NIMBO-24	2-way passive loudspeaker for surface mounting (2x 4" woofers and 1" tweeter). Capable of working at	516,79 €
both 4 Ωand 16Ωin low impedance, featuring the front switch locatedbehind the logo. 80 WRMS. Suitable for outdoor applications, with a wide dispersion pattern and IP-44 rating. White color. Dimensions 370 x 180 x 180 mm. / 14.56"x7.08"x7.08". Weight 3 kg. / 6,61 lb. Delivered by units. Price per unit.
	656,32 €
	209 300 Ft
	265 811 Ft



	CNIMBO24BK	NIMBO-24	2-way passive loudspeaker for surface mounting (2x 4" woofers and 1" tweeter). Capable of working at	516,79 €
both 4 Ωand 16Ωin low impedance, featuring the front switch locatedbehind the logo. 80 WRMS. Suitable for outdoor applications, with a wide dispersion pattern and IP-44 rating. Black color.
Dimensions 370 x 180 x 180 mm. / 14.56"x7.08"x7.08". Weight 3 kg. / 6,61 lb..Delivered by units. Price per unit.
	656,32 €
	209 300 Ft
	265 811 Ft



	CNIMBO24GD	NIMBO-24	2-way passive loudspeaker for surface mounting (2x 4" woofers and 1" tweeter). Capable of working at	516,79 €
both 4 Ωand 16Ωin low impedance, featuring the front switch locatedbehind the logo. 80 WRMS. Suitable for outdoor applications, with a wide dispersion pattern and IP-44 rating. Gold color.
Dimensions 370 x 180 x 180 mm. / 14.56"x7.08"x7.08". Weight 3 kg. / 6,61 lb. Delivered by units. Price per unit.
	656,32 €
	209 300 Ft
	265 811 Ft



	NEW!
	CNIMBO24TN
	NIMBO-24
	2-way passive loudspeaker for surface mounting (2x 4" woofers and 1" tweeter). Capable of working at both 4 Ωand 16Ωin low impedance, featuring the front switch locatedbehind the logo. 80 WRMS. Suitable for outdoor applications, with a wide dispersion pattern and IP-44 rating. Titanium color.
Dimensions 370 x 180 x 180 mm. / 14.56"x7.08"x7.08". Weight 3 kg. / 6,61 lb. Delivered by units. Price per unit.
	516,79 €
	656,32 €
	209 300 Ft
	265 811 Ft




	CNIMBO24CR	NIMBO-24	NIMBO-24 cabinet RAL customization (black grill and bracket). MOQ: 8 units. Delivery time: 45 days.	594,07 €
Dimensions 370 x 180 x 180 mm. / 14.56"x7.08"x7.08". Weight 3 kg. / 6,61 lb. Delivered by units. Price per unit.
	754,47 €
	240 600 Ft
	305 562 Ft



	CNIMBO26WH	NIMBO-26	2-way passive loudspeaker for surface mounting (2x 6" woofers and 1" tweeter). Capable of working at	938,27 €
both 4 Ωand 16Ωin low impedance, featuring the front switch locatedbehind the logo. 140 WRMS. Suitable for outdoor applications, with a wide dispersion pattern and IP-44 rating. White color.
Dimensions 542,5 x 261 x 269 mm. / 21.35"x 10.27"x 10.59". Weight 8,5 kg. / 18.73 lb. Delivered by units. Price per unit.
	1 191,60 €
	380 000 Ft
	482 600 Ft



	CNIMBO26BK	NIMBO-26	2-way passive loudspeaker for surface mounting (2x 6" woofers and 1" tweeter). Capable of working at	938,27 €
both 4 Ωand 16Ωin low impedance, featuring the front switch locatedbehind the logo. 140 WRMS. Suitable for outdoor applications, with a wide dispersion pattern and IP-44 rating. Black color.
Dimensions 542,5 x 261 x 269 mm. / 21.35"x 10.27"x 10.59". Weight 8,5 kg. / 18.73 lb. Delivered by units. Price per unit.
	1 191,60 €
	380 000 Ft
	482 600 Ft



	CNIMBO26GD	NIMBO-26	2-way passive loudspeaker for surface mounting (2x 6" woofers and 1" tweeter). Capable of working at	938,27 €
both 4 Ωand 16Ωin low impedance, featuring the front switch locatedbehind the logo. 140 WRMS. Suitable for outdoor applications, with a wide dispersion pattern and IP-44 rating. Gold color.
Dimensions 542,5 x 261 x 269 mm. / 21.35"x 10.27"x 10.59". Weight 8,5 kg. / 18.73 lb. Delivered by units. Price per unit.
	1 191,60 €
	380 000 Ft
	482 600 Ft



	NEW!
	CNIMBO26TN
	NIMBO-26
	2-way passive loudspeaker for surface mounting (2x 6" woofers and 1" tweeter). Capable of working at both 4 Ωand 16Ωin low impedance, featuring the front switch locatedbehind the logo. 140 WRMS. Suitable for outdoor applications, with a wide dispersion pattern and IP-44 rating. Titanium color.
Dimensions 542,5 x 261 x 269 mm. / 21.35"x 10.27"x 10.59". Weight 8,5 kg. / 18.73 lb. Delivered by units. Price per unit.
	938,27 €
	1 191,60 €
	380 000 Ft
	482 600 Ft



	NEW!
	CNIMBO26CR

[image: ]

	NIMBO-26
	NIMBO-26 cabinet RAL customization (black grill and bracket). MOQ: 8 units. Delivery time: 45 days. Dimensions 542,5 x 261 x 269 mm. / 21.35"x 10.27"x 10.59". Weight 8,5 kg. / 18.73 lb. Delivered by units. Price per unit.
	1 077,53 €
	1 368,46 €
	436 400 Ft
	554 228 Ft


Ref.
Name
NIMBO Merchandising
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	NEW!
	CMNIMBOSCREW
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	NIMBOSCREW

[image: ]
	Set of 24 small precision screwdrivers, with silk-screened NIMBO logo. Presented in an ABS magnetic box with snap-opening. Dimensions: 60 x 160 x 15 mm / 2.32" x 6.29" x 0.59". Weight:220gr / 0,48 lb.Price per unit.
	24,20 €
	30,73 €
	9 800 Ft
	12 446 Ft


Ref.
Name
ARQISi SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CARQIS105IB	ARQIS 105iBK	2-way (5,25" woofer and 1" HF tweeter) wooden loudspeaker cabinet with a compact format and long	260,99 €
term reliability, featuring 70 WRMS @ 8 Ω. 280W Peak power. Its smart wall bracket (included), allows for pan&tilt adjustment, employing a single screw for fastening. Double INPUT/STACK connector, Euroblock type, with security attachment screws, and metal safety sling included. 150ºx130º dispersion pattern. Dimensions (WxHxD) 186 x 280 x 210 mm / 7,32 x 11,02 x 8,26 in
Weight 3.6 kg. Black color
	331,45 €
	105 700 Ft
	134 239 Ft



	CARQIS105IW	ARQIS 105iWH	2-way (5,25" woofer and 1" HF tweeter) wooden loudspeaker cabinet with a compact format and long	260,99 €
term reliability, featuring 70 WRMS @ 8 Ω. 280W Peak power. Its smart wall bracket (included), allows for pan&tilt adjustment, employing a single screw for fastening. Double INPUT/STACK connector, Euroblock type, with security attachment screws, and metal safety sling included. 150ºx130º dispersion pattern. Dimensions (WxHxD) 186 x 280 x 210 mm / 7,32 x 11,02 x 8,26 in .Weight 3.6 kg
White color
	331,45 €
	105 700 Ft
	134 239 Ft





	CARQIS106IB	ARQIS 106iBK	2-way (6" woofer and 1" rotable HF Compressor Driver) wooden loudspeaker cabinet with a compact	356,30 €
format and long term reliability, featuring 120 WRMS@8Ω. 480W Peak power. Its smart wall bracket (included), allows for pan&tilt adjustment, employing a single screw for fastening. Double INPUT/STACK connector, Euroblock type, with security attachment screws, and metal safety sling included. 140ºx160º dispersion pattern. Dimensions (WxHxD) 216x350x240mm / 8.50"x13.78"x9.45". Weight 7,4 kg / 16.31 lb
Black color
	452,50 €
	144 300 Ft
	183 261 Ft



	CARQIS106IW	ARQIS 106iWH	2-way (6" woofer and 1" rotable HF Compressor Driver) wooden loudspeaker cabinet with a compact	356,30 €
format and long term reliability, featuring 120 WRMS@8Ω.480W Peak power. Its smart wall bracket (included), allows for pan&tilt adjustment, employing a single screw for fastening. Double INPUT/STACK connector, Euroblock type, with security attachment screws, and metal safety sling included. 140ºx160º dispersion pattern. Dimensions (WxHxD) 216x350x240mm / 8.50"x13.78"x9.45". Weight 7,4 kg / 16.31 lb. White color
	452,50 €
	144 300 Ft
	183 261 Ft



	CARQIS108IB	ARQIS 108iBK	2-way (8" woofer and 1" HF Compression Driver) wooden loudspeaker cabinet with a compact format,	421,48 €
stylish aesthetics, excellent sound quality and long term reliability, featuring 150 WRMS @ 8 Ω. 600W Peak power. Its smart wall bracket (included), allows for pan&tilt adjustment, employing a single screw for fastening. 130⁰x130⁰ dispersion pattern. Dimensions (WxHxD) 244 x 390 x 280 mm / 9.60" x 15.35" x 11.02". Weight 8,4 kg / 18.52 lb. Black color.
	535,28 €
	170 700 Ft
	216 789 Ft



	CARQIS108IW	ARQIS 108iWH	2-way (8" woofer and 1" HF Compression Driver) wooden loudspeaker cabinet with a compact format,	421,48 €
stylish aesthetics, excellent sound quality and long term reliability, featuring 150 WRMS @ 8 Ω. 600W Peak power. Its smart wall bracket (included), allows for pan&tilt adjustment, employing a single screw for fastening. 130⁰x130⁰ dispersion pattern. Dimensions (WxHxD) 244 x 390 x 280 mm / 9.60" x 15.35" x 11.02". Weight 8,4 kg / 18.52 lb. White color
	535,28 €
	170 700 Ft
	216 789 Ft



	CARQIS110IB	ARQIS 110iBK	2-way (10" woofer and 1" rotable HF Compression Driver) wooden loudspeaker cabinet with a compact	559,01 €
format, stylish aesthetics and long term reliability, featuring 300 WRMS @ 8 ohm. 1200W Peak power. 35 mm mount socket and 8 x M10 rigging points, allowing for horizontal or vertical mounting options (110°x 110° dispersion pattern). Dimensions (WxHxD) 359x495x310mm / 14.13"x19.49"x13.86".
Weight 14,8 kg / 32.63 lb
Black color. Bracket not included. Optional ARQ110UB, TRIPO and SR12 accessories.
	709,95 €
	226 400 Ft
	287 528 Ft



	CARQIS110IW	ARQIS 110iWH	2-way (10" woofer and 1" rotable HF Compression Driver) wooden loudspeaker cabinet with a compact	559,01 €
format, stylish aesthetics and long term reliability, featuring 300 WRMS @ 8 ohm. 1200W Peak power. 35 mm mount socket and 8 x M10 rigging points, allowing for horizontal or vertical mounting options (110°x 110° dispersion pattern). Dimensions (WxHxD) 359x495x310mm / 14.13"x19.49"x13.86".
Weight 14,8 kg / 32.63 lb
White color. Bracket not included. Optional ARQ110UB, TRIPO and SR12 accessories.
	709,95 €
	226 400 Ft
	287 528 Ft



	CARQIS112IB	ARQIS 112iBK	2-way ( 12" woofer and 1,4" rotable HF Compression Driver) wooden loudspeaker cabinet with a	823,70 €
compact format, stylish aesthetics and long term reliability, featuring 500 WRMS @ 8 Ω. 2000W Peak power. 35 mm mount socket and 8 x M10 rigging points, allowing for horizontal or vertical mounting options (120°x 110° dispersion pattern). Dimensions (WxHxD)416x565x352mm / 16.37"x22.24"x13.86". Weight 20,0 kg / 44.09 lb. Black color. Bracket not included. Optional ARQ112UB, TRIPO and SR12 accessories.
	1 046,10 €
	333 600 Ft
	423 672 Ft



	CARQIS112IW	ARQIS 112iWH	2-way ( 12" woofer and 1,4" rotable HF Compression Driver) wooden loudspeaker cabinet with a	823,70 €
compact format, stylish aesthetics and long term reliability, featuring 500 WRMS @ 8 Ω. 2000W Peak power. 35 mm mount socket and 8 x M10 rigging points, allowing for horizontal or vertical mounting options (120°x 110° dispersion pattern). Dimensions (WxHxD)416x565x352mm / 16.37"x22.24"x13.86". Weight 20,0 kg / 44.09 lb. White color. Bracket not included. Optional ARQ112UB, TRIPO and SR12 accessories.
	1 046,10 €
	333 600 Ft
	423 672 Ft



	CARQIS205IB	ARQIS 205iBK	2-way (2x 5,25" woofer and 1" HF rotable Compression Driver) wooden loudspeaker cabinet with a	415,56 €
compact format and long term reliability, featuring 140 WRMS @ 8 Ω. 560W Peak power. Double INPUT/STACK connector, Euroblock + Speakon© type, 8 x M8 cabinet flying points, metal safety sling included. Its "U" shape wall bracket (included) allows for tilt adjustment. 150º x 40º dispersion pattern. Dimensions (WxHxD) 480x186x210mm / 18.89"x7.32"x8.26". Weight 8.4 kg. / 18.52 lb
Black color.
	527,76 €
	168 300 Ft
	213 741 Ft




	CARQIS205IW	ARQIS 205iWH	2-way (2x 5,25" woofer and 1" HF rotable Compression Driver) wooden loudspeaker cabinet with a	415,56 €
compact format and long term reliability, featuring 140 WRMS @ 8 Ω. 560W Peak power. Double INPUT/STACK connector, Euroblock + Speakon© type, 8 x M8 cabinet flying points, metal safety sling included. Its "U" shape wall bracket (included) allows for tilt adjustment. 150º x 40º dispersion pattern. Dimensions (WxHxD) 480x186x210mm / 18.89"x7.32"x8.26". Weight 8.4 kg. / 18.52 lb. White color.
	527,76 €
	168 300 Ft
	213 741 Ft



	CARQIS208IB	ARQIS 208iBK	2-way (2 x 8" woofer and 1" HF Compression Driver) wooden loudspeaker cabinet with a compact	639,26 €
format and long term reliability, featuring 300 WRMS @ 8 Ω. 1200W Peak power. Double INPUT/STACK connector, Euroblock + Speakon© type, 8 x M8 cabinet flying points, metal safety sling included.
Its "U" shape wall bracket (included) allows for tilt adjustment. 130ºx30º dispersion pattern. Dimensions(WxHxD) 610x244x280mm / 24.01"x9.60"x11.02". Weight 14.4 kg / 31.74 lb. Black color.
	811,86 €
	258 900 Ft
	328 803 Ft



	CARQIS208IW	ARQIS 208iWH	2-way (2 x 8" woofer and 1" HF Compression Driver) wooden loudspeaker cabinet with a compact	639,26 €
format and long term reliability, featuring 300 WRMS @ 8 Ω. 1200W Peak power. Double INPUT/STACK connector, Euroblock + Speakon© type, 8 x M8 cabinet flying points, metal safety sling included.
Its "U" shape wall bracket (included) allows for tilt adjustment. 130ºx30º dispersion pattern. Dimensions(WxHxD) 610x244x280mm / 24.01"x9.60"x11.02" . Weight 14.4 kg / 31.74 lb. White color.
	811,86 €
	258 900 Ft
	328 803 Ft


Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CLABI1C100I	LABI1-C100i	LABI1-C100i is a versatile and discreet column loudspeaker, designed for indoor and outdoor fixed	1 374,57 €
installations and portable applications.
It features twelve 3” drivers with 0.75” neodymium voice coil each one, 300W AES. Its versatile profile allows the column to be installed in several ways such on the LABI subwoofers, on wall, pole, truss, etc. thanks to LABI1 accessories. Stand alone or combined with other LABI1-C100i and LABI1-SP18p to create a complete powerful plug & play solution. Dimensions: 89 x 1000 x 117 mm / 3.5” x 39.4” x 4.6”. Weight: 7.8 kg / 17.2 lb.
	1 745,70 €
	556 700 Ft
	707 009 Ft


Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CDROP6BK	DROP6	ECLER DROP6 is a 2-way 6.5”, 75W@8ohm pendant loudspeaker with a stylish design, including a	321,23 €
70/100V line transformer with 60/30/15 and 7,5W power selections, available at both high and low impedance levels. Dimensions (without accessories) Ø270mm x 355mm(H) / Ø10.6 in. x 14 in. (H). Weight 4.2 Kg / 9.26 lb. Stripped wire connection (5m). Black colour.
	407,97 €
	130 100 Ft
	165 227 Ft



	CDROP6WH	DROP6	ECLER DROP6 is a 2-way 6.5”, 75W@8ohm pendant loudspeaker with a stylish design, including a	321,23 €
70/100V line transformer with 60/30/15 and 7,5W power selections, available at both high and low impedance levels. Dimensions (without accessories) Ø270mm x 355mm(H) / Ø10.6 in. x 14 in. (H). Weight 4.2 Kg / 9.26 lb. 2x stripped wire connection (5m). White colour.
	407,97 €
	130 100 Ft
	165 227 Ft


Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CZEN15GR	ZEN-15	The new ZEN-15 in-ground loudspeaker with an elegant rounded rock shape seamlessly blends the	399,51 €
world of audio technology with the aesthetics of nature. Includes a 5,25" woofer and a 1" tweeter delivering 70W RMS @ 8ohm and 60W RMS @ 70/100V. This discreet outdoor audio solution effortlessly integrates into outdoor environments, providing a harmonious balance between functionality and visual appeal.Grey color. Dimensions 410 x 260 x 289mm / 16.14 x 10.23 x 11,37 in. Weight 4.4Kg / 9.7lb
	507,37 €
	161 800 Ft
	205 486 Ft



	CZEN15SD	ZEN-15	The new ZEN-15 in-ground loudspeaker with an elegant rounded rock shape seamlessly blends the	399,51 €
world of audio technology with the aesthetics of nature. Includes a 5,25" woofer and a 1" tweeter delivering 70W RMS @ 8ohm and 60W RMS @ 70/100V. Crafted to resemble a rugged, weathered stone, this discreet outdoor audio solution effortlessly integrates into outdoor environments, providing a harmonious balance between functionality and visual appeal.Sand color. Dimensions 410 x 260 x 289mm / 16.14 x 10.23 x 11,37 in. Weight 4.4Kg / 9.7lb
	507,37 €
	161 800 Ft
	205 486 Ft


Ref.	Name	RRP €	RRP €	RRP €	RRP €


	CIG108	IG108	Weatherproof loudspeaker (IP65) with an omni-directional horizontal dispersion pattern (360º). 8"	478,77 €
Kevlar woofer and 1" ACCW silk tweeter. 100 WRMS @ 8Ω, suitable for 70/100V ( 7.5/15/30/60 W @ 100V ). Frequency response 50Hz to 23kHz.Security ground bracket included. It is ideal for music and message applications in outdoor areas. Dimensions 360 x 392.5 mm. Weight 8.5 kg
	608,03 €
	193 900 Ft
	246 253 Ft


COMMERCIAL LOUDSPEAKERS
Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF




	CTRAIL103BK	TRAIL103BK	3" lamp style loudspeaker cabinet, with high Impedance (15W and 30W taps) and Low Impedance (15	234,81 €
WRMS @4Ω) connections. Includes 3 different installation system accesories for ceiling light rails, surface mount and truss mount. Dimensions (without arm) Ø 96mm x 110mm. Weight 1kg Black colour.
Delivered by units. Price per unit.
	298,21 €
	95 100 Ft
	120 777 Ft



	CTRAIL103WH	TRAIL103WH	3" lamp style loudspeaker cabinet, with high Impedance (15W and 30W taps) and Low Impedance (15	234,81 €
WRMS @4Ω) connections. Includes 3 different installation system accesories for ceiling light rails, surface mount and truss mount. Dimensions (without arm) Ø 96mm x 110mm. Weight 1kg White colour.
Delivered by units. Price per unit.
	298,21 €
	95 100 Ft
	120 777 Ft


Ref.
Name
eAMBIT SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	EOL
	CEAMB103BK

[image: ]

	eAMBIT103BK
	Ultra compact 2-way (3.5” woofer and 0.5" tweeter) loudspeaker cabinet with neutral an discreet design, suitable for 70/100V (2.5/5/7.5/15 W) and low impedance (25 WRMS @8Ω) audio lines. IP54 certified. Includes on-wall hardware, safety sling, screws and wrench for fast installation.Dimensions (without accessories) 120 x 120 x 117 mm. Weight 1,275kg Black color.
Delivered by master carton of 2 units. Price per unit.
	70,37 €
	89,37 €
	28 500 Ft
	36 195 Ft



	EOL
	CEAMB103WH

[image: ]

	eAMBIT103WH
	Ultra compact 2-way (3.5” woofer and 0.5" tweeter) loudspeaker cabinet with neutral an discreet design, suitable for 70/100V (2.5/5/7.5/15 W) and low impedance (25 WRMS @8Ω) audio lines. IP54 certified. Includes on-wall hardware, safety sling, screws and wrench for fast installation.Dimensions (without accessories) 120 x 120 x 117 mm. Weight 1,275kg White color.
Delivered by master carton of 2 units. Price per unit.
	70,37 €
	89,37 €
	28 500 Ft
	36 195 Ft


Ref.
Name
AMBIT SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	NEW!
	CAMBIT13BK

[image: ]

	AMBIT-13
	Ultra compact 2-way (3.5” woofer and 0.5" tweeter) loudspeaker cabinet with neutral an discreet design, suitable for 70/100V (2.5/5/7.5/15 W) and low impedance (25 WRMS @8Ω) audio lines. IP54 certified. Includes on-wall hardware, safety sling, screws and wrench for fast installation.Dimensions (without accessories) 120 x 120 x 117 mm. Weight 1,275kg Black color.
Delivered by master carton of 2 units. Price per unit.
	74,32 €
	94,39 €
	30 100 Ft
	38 227 Ft



	NEW!
	CAMBIT13WH
[image: ]

	AMBIT-13
	Ultra compact 2-way (3.5” woofer and 0.5" tweeter) loudspeaker cabinet with neutral an discreet design, suitable for 70/100V (2.5/5/7.5/15 W) and low impedance (25 WRMS @8Ω) audio lines. IP54 certified. Includes on-wall hardware, safety sling, screws and wrench for fast installation.Dimensions (without accessories) 120 x 120 x 117 mm. Weight 1,275kg White color.
Delivered by master carton of 2 units. Price per unit.
	74,32 €
	94,39 €
	30 100 Ft
	38 227 Ft



	NEW!
	CAMBIT16BK
[image: ]

	AMBIT-16
	Ultra compact 2-way (6.5” woofer and 1" tweeter) loudspeaker cabinet with neutral an discreet design, suitable for 70/100V (5/7.5/15/30 W) and low impedance(50 WRMS @8Ω) audio lines. IP54 certified. Includes on-wall hardware, safety sling, screws and wrench for fast installation.Dimensions (without accessories) 210 x 210 x 160 mm. Weight 2,75kg Black color.
Delivered by master carton of 2 units. Price per unit.
	122,47 €
	155,54 €
	49 600 Ft
	62 992 Ft



	NEW!
	CAMBIT16WH
[image: ]

	AMBIT-16
	Ultra compact 2-way (6.5” woofer and 1" tweeter) loudspeaker cabinet with neutral an discreet design, suitable for 70/100V (5/7.5/15/30 W) and low impedance(50 WRMS @8Ω) audio lines. IP54 certified. Includes on-wall hardware, safety sling, screws and wrench for fast installation. Dimensions (without accessories) 210 x 210 x 160 mm. Weight 2,75kg White color.
Delivered by master carton of 2 units. Price per unit.
	122,47 €
	155,54 €
	49 600 Ft
	62 992 Ft



	NEW!
	CAMBIT18BK
[image: ]

	AMBIT-18
	Ultra compact 2-way (8” woofer and 1,18" tweeter) loudspeaker cabinet with neutral an discreet design, suitable for 70/100V (60 W) and low impedance(75 WRMS @8Ω) audio lines. IP54 certified. Includes on-wall hardware, safety sling, screws and wrench for fast installation.Dimensions (without accessories) 258 x 258 x 225 mm. Weight 5.6k.g Black color.
Delivered by master carton of 2 units. Price per unit.
	251,85 €
	319,85 €
	102 000 Ft
	129 540 Ft



	NEW!
	CAMBIT18WH
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	AMBIT-18
	Ultra compact 2-way (8” woofer and 1,18" tweeter) loudspeaker cabinet with neutral an discreet design, suitable for 70/100V (60 W) and low impedance(100 WRMS @8Ω) audio lines. IP54 certified. Includes on-wall hardware, safety sling, screws and wrench for fast installation.Dimensions (without accessories) 258 x 258 x 225 mm. Weight 5.6k.g. White color.
Delivered by master carton of 2 units. Price per unit.
	251,85 €
	319,85 €
	102 000 Ft
	129 540 Ft


Ref.
Name
eMOTUS SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CEMOTUS3ODWH	eMOTUS3ODWH	3" woofer (25 WRMS @ 8Ω) loudspeaker cabinet ready for outdoor installation(IP65). Suitable for	93,33 €
70/100V and low impedance(8Ω) audio lines. Includes wall bracket and security steel cable. Dimensions (without accessories) 132x132x117 mm. Weight 1.3 kg White colour.
Price per unit, sold in pairs.
	118,53 €
	37 800 Ft
	48 006 Ft



	CEMOTUS3ODBK

[image: ]

	eMOTUS3ODBK
	3" woofer (25 WRMS @ 8Ω) loudspeaker cabinet ready for outdoor installation(IP65). Suitable for 70/100V and low impedance(8Ω) audio lines. Includes wall bracket and security steel cable.
Dimensions (without accessories) 132x132x117 mm. Weight 1.3 kg Black colour. Price per unit, sold in pairs.
	93,33 €
	118,53 €
	37 800 Ft
	48 006 Ft

	
	
	
	

	CEMOTUS5PBWC

[image: ] [image: ]

	eMOTUS5PBWH
	Stereo loudspeaker kit (2 x 25 WRMS @ 8Ω) including an active and a passive cabinet. eMOTUS5PBBK performs BT connection, balanced and unbalanced audio inputs. Includes an IR remote control and 0- 10VDC remote port. Features: source selection, 2 band tone control, stereo/mono switch, auto stand- by and wall bracket and security steel cable. Dimensions 173x185x180mm. Weight 2.1 kg. White colour.
Delivered by kit (active + passive loudspeakers). Price per kit.
	356,30 €
	452,50 €
	144 300 Ft
	183 261 Ft


Ref.
Name
eUC SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF

	CEMOTUS5PWHC	eMOTUS5PWH	Stereo loudspeaker kit (2 x 25 WRMS @ 8Ω) including an active and a passive cabinet and performing 2	273,09 €
audio inputs: balanced and unbalanced. Suitable for low impedance audio lines, includes source selection, 2 band tone control, stereo/mono switch, auto stand-by and wall bracket and security steel cable. Dimensions (without accessories) 173x185x180mm. Weight 2.1 kg White colour.
Delivered by kit (active + passive loudspeakers). Price per kit.
	346,82 €
	110 600 Ft
	140 462 Ft



	NEW!
	CEMOTUS5PBKC
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	eMOTUS5PBK
	Stereo loudspeaker kit (2 x 25 WRMS @ 8Ω) including an active and a passive cabinet and performing 2 audio inputs: balanced and unbalanced. Suitable for low impedance audio lines, includes source selection, 2 band tone control, stereo/mono switch, auto stand-by and wall bracket and security steel cable. Dimensions (without accessories) 173x185x180mm. Weight 2.1 kg Black colour.
Delivered by kit (active + passive loudspeakers). Price per kit.
	273,09 €
	346,82 €
	110 600 Ft
	140 462 Ft



	CEMOTUS5ODBK	eMOTUS5ODBK	5" woofer and 1" tweeter (40 WRMS @ 8Ω) loudspeaker cabinet ready for outdoor installation(IP65).	150,62 €
Suitable for 100V (3,75/7,5/15/30W) and low impedance(8Ω) audio lines. Includes wall bracket and security steel cable. Dimensions (without accessories) 173x181x180mm. Weight 2.4 kg Black colour. Price per unit, sold in pairs.
	191,28 €
	61 000 Ft
	77 470 Ft



	CEMOTUS5ODWH	eMOTUS5ODWH	5" woofer and 1" tweeter (40 WRMS @ 8Ω) loudspeaker cabinet ready for outdoor installation(IP65).	150,62 €
Suitable for 100V (3,75/7,5/15/30W) and low impedance(8Ω) audio lines. Includes a wall bracket and security steel cable. Dimensions (without accessories) 173x181x180mm. Weight 2.4 kg White colour. Price per unit, sold in pairs.
	191,28 €
	61 000 Ft
	77 470 Ft



	NEW!
	CEMOTUS5O16B
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	eMOTUS5O16
	5" woofer and 1" tweeter (40 WRMS @ 16Ω) loudspeaker cabinet ready for outdoor installation(IP65). Suitable for low impedance(16Ω) audio lines. Includes a wall bracket and security steel cable.
Dimensions (without accessories) 173x181x180mm. Weight 2.4 kg. Black colour. Price per unit, sold in pairs.
	129,63 €
	164,63 €
	52 500 Ft
	66 675 Ft



	NEW!
	CEMOTUS5O16W
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	eMOTUS5O16
	5" woofer and 1" tweeter (40 WRMS @ 16Ω) loudspeaker cabinet ready for outdoor installation(IP65). Suitable for low impedance(16Ω) audio lines. Includes a wall bracket and security steel cable.
Dimensions (without accessories) 173x181x180mm. Weight 2.4 kg White colour. Price per unit, sold in pairs.
	129,63 €
	164,63 €
	52 500 Ft
	66 675 Ft



	CEMOTUS8ODBK	eMOTUS8ODBK	8" woofer and 1" tweeter (100 WRMS @ 8Ω) loudspeaker cabinet ready for outdoor installation(IP65).	297,04 €
Suitable for 70/100V (3,75/7,5/15/30W/60W) and low impedance(8Ω) audio lines. Includes a wall bracket and security steel cable. Dimensions (without accessories) 268x242x264mm. Weight 4.25 kg Black colour.
Price per unit, sold in pairs.
	377,24 €
	120 300 Ft
	152 781 Ft



	CEMOTUS8ODWH	eMOTUS8ODWH	8" woofer and 1" tweeter (100 WRMS @ 8Ω) loudspeaker cabinet ready for outdoor installation(IP65).	297,04 €
Suitable for 70/100V (3,75/7,5/15/30W/60W) and low impedance(8Ω) audio lines. Includes a wall bracket and security steel cable. Dimensions (without accessories) 268x242x264mm. Weight 4.25 kg White colour.
Price per unit, sold in pairs.
	377,24 €
	120 300 Ft
	152 781 Ft

	
	
	
	



	CEUC106BK	eUC106BK	Spherical pendant loudspeaker featuring a 6,5" woofer, 0.5" tweeter. 40 WRMS @ 8Ω and 70/100V	149,63 €
transformer (32/ 16/ 8/ 4 W @ 100V). Dimensions (without accessories) ø270 x 215 (H). Weight 3 kg Stripped wire connection (3m). Black colour.
	190,03 €
	60 600 Ft
	76 962 Ft




Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF
Ref.
Name
ARQISi SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF

	CEUC106	eUC106WH	Spherical pendant loudspeaker featuring a 6,5" woofer, 0.5" tweeter. 40 WRMS @ 8Ω and 70/100V	149,63 €
transformer.(32/ 16/ 8/ 4 W @ 100V). Dimensions (without accessories) ø270 x 215 (H). Weight 3 kg Stripped wire connection (3m). White colour.
	190,03 €
	60 600 Ft
	76 962 Ft


Ref.
Name
eCMP SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CECMP8	eCMP8	150W high efficiency musical projector ready for outdoor applications due to its waterproof and sun	448,64 €
screening building material (IP56). It performs an 8’’ LF driver and 1,4’’ HF coaxial driver, 150W @ 8Ω nominal power and 70/100V line transformer with 37, 5/75/150W/ 8Ω power options.
Dimensions: WxHxD: 300 x 302 x 334mm /11.8” x 11.9” x 13.2”
Weight: 11,0 kg / 24.3 lb
	569,78 €
	181 700 Ft
	230 759 Ft



	CECMP12	eCMP12	300W high efficiency musical projector ready for outdoor applications due to its waterproof and sun	721,48 €
screening building material (IP56). It performs an 12’’ LF driver and 1,7’’ HF coaxial driver, 300W @ 8Ω nominal power and 70/100V line transformer with 50/100/200W/8Ω power options.
Dimensions: WxHxD: 407 x 410 x 378mm / 16.0” x 16.1” x 14.9”
Weight: 20,0 kg / 44.1 lb
	916,28 €
	292 200 Ft
	371 094 Ft


SUBWOOFERS



	NEW!
	CKICKSB18BK
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	KICK-SB18
	As the first Ecler outdoor subwoofer, the new KICK-SB18 features 1x8” woofers perfectly positioned to maximize the low frequency response while reducing the vibrations on the acoustic enclosure. It delivers 350 WRMS at 8Ω ready to be wall-mounted with the included bracket or positioned vertically and horizontally when needed. Dimensions TBC. Weight TBC
Black color.
	701,48 €
	890,88 €
	284 100 Ft
	360 807 Ft



	CKICKSB28BK	KICK-SB28	As the first Ecler outdoor subwoofer, the new KICK-SB28 features 2x8” woofers perfectly positioned to	1 315,31 €
maximize the low frequency response while reducing the vibrations on the acoustic enclosure. It delivers 700 WRMS at 4Ω ready to be wall-mounted with the included bracket or positioned vertically and horizontally when needed. Dimensions (WxHxD) 660 x 450 x 250 mm / 255,98 x 17,71 x 9,84 in. Weight 23Kg/50.7lb
Black color.
	1 670,44 €
	532 700 Ft
	676 529 Ft



	CEDGESB110P	EDGE-SB110P	Powerful bass sound in a compact size EDGE subwoofer is perfectly designed for small available spaces	450,62 €
like underneath restaurant seats or wall-mounted in a corner with the included bracket. This powered subwoofer of 181 mm high incorporates a 10” driver, 50Hz to 250Hz variable low pass filter, phase inverter and an amplified power output of 120W.Black color. Dimensions (WxHxD) 635 x 400 x 178 mm
/ 23,62 x 15,74 x 7 in. Weight 11,25Kg & 24,8 lb
	572,28 €
	182 500 Ft
	231 775 Ft



	NEW!
	CEDGESB10P21
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	EDGE-SB10P21
	EDGE-SB10P21 is a compact powered 2.1 device, including in a single enclosure a powered subwoofer and a stereo amplifier for full range external speakers or "satellites", as well as a number of additional components to control and process the audio signal.Powerful bass sound in a compact size EDGE subwoofer is perfectly designed for small available spaces like underneath restaurant seats or wall- mounted in a corner with the included bracket.Black color. Dimensions (WxHxD) 635 x 400 x 178 mm / 23,62 x 15,74 x 7 in. Weight 11,25Kg & 24,8 lb
	600,99 €
	763,25 €
	243 400 Ft
	309 118 Ft




	CARQISSB6TIB	ARQISSB6TiBK	Wooden wall-mount subwoofer reinforcement cabinet, featuring a 6,5" driver and a passive 6,5"	559,01 €
radiator. 480W peak power, 120 WRMS power @ 8 ohm and integrated 70/100V line transformer with 60 and 120W taps. Internal LPF with OFF, 120HZ and 150 HZ cut-off frequency selections. Installation U- bracket included. Dimensions (WxHxD) 250x390x130mm / 9.84"x15.35"x5.12". Weight 8,2 kg / 18.07 lb Black color.
	709,95 €
	226 400 Ft
	287 528 Ft



	CARQISSB6TIW	ARQISSB6TiWH	Wooden wall-mount subwoofer reinforcement cabinet, featuring a 6,5" driver and a passive 6,5"	559,01 €
radiator. 480W peak power, 120 WRMS power @ 8 ohm and integrated 70/100V line transformer with 60 and 120W taps. Internal LPF with OFF, 120HZ and 150 HZ cut-off frequency selections. Installation U- bracket included. Dimensions (WxHxD) 250x390x130mm / 9.84"x15.35"x5.12". Weight 8,2 kg / 18.07 lb White color.
	709,95 €
	226 400 Ft
	287 528 Ft



	CARQISSB10IB	ARQIS SB10iBK	Wooden wall-mount subwoofer reinforcement cabinet with a slim and compact format and long term	569,88 €
reliability, featuring a 10" driver (150 WRMS @ 8 ohm, 600W peak power) and internal LPF (OFF/ 120Hz/150Hz). Euroblock connector, wall mount and 12 x M8 rigging points included. Dimensions (WxHxD) 600x442x228mm / 23.62"x17.40"8.97". Weight 16,6 kg / 36.37 lb.
Black color.
	723,74 €
	230 800 Ft
	293 116 Ft




	CARQISSB10IW	ARQIS SB10iWH	Wooden wall-mount subwoofer reinforcement cabinet with a slim and compact format and long term	569,88 €
reliability, featuring a 10" driver (150 WRMS @ 8 ohm, 600W peak power) and internal LPF (OFF/ 120Hz/150Hz). Euroblock connector, wall mount and 12 x M8 rigging points included. Dimensions (WxHxD) 600x442x228mm / 23.62"x17.40"8.97". Weight 16,6 kg / 36.37 lb.
White color.
	723,74 €
	230 800 Ft
	293 116 Ft



	CARQISSB12IB	ARQIS SB12iBK	Wooden sub-woofer reinforcement cabinet with a compact format and long term reliability, featuring	761,48 €
300 WRMS @ 8 Ω and a 12" LF driver. 1200W Peak power. Double INPUT/STACK connector, Speakon© type.
8 x M8 rigging points included. Dimensions (WxHxD) 445 x 445 x 375 mm / 17.51 x 17.51 x 14.76 in. Weight 23 kg / 50,70 lb. Available only in black color.
	967,08 €
	308 400 Ft
	391 668 Ft



	CARQISSB15IB	ARQIS SB15iBK	Wooden sub-woofer reinforcement cabinet with a compact format and long term reliability, featuring	964,20 €
600 WRMS @ 8 Ω and a 15" LF driver. 2400W Peak power. Double INPUT/STACK connector, Speakon© type.
35 mm top-hat pole mount socket and 8 x M8 rigging points included. Dimensions (WxHxD) 534 x 525 x 460 mm / 21.02 x 20.67 x 18.11 in. Weight 32 kg / 70,54 lb. Available only in black color.
	1 224,53 €
	390 500 Ft
	495 935 Ft


Ref.	Name	Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár


	CTRAILSB6TBK	TRAILSB6TBK	Wooden subwoofer reinforcement cabinet with a very compact format, featuring a 6,5" driver, 60	467,65 €
WRMS @ 8Ω, 70/100V line transformer (7.5/15/30/60 W), and internal Low Pass Filter(150Hz / OFF). Specifically designed to fulfil permanent installation requirements: concealed in false ceilings or partition walls, on walls' surface, etc. Installation accessories included. Dimensions 200x200x320 mm. Weight 6,3kg
Available only in black finish. Delivered by units. Price per unit.
	593,92 €
	189 400 Ft
	240 538 Ft


Ref.
Name
LABI1 SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CLABI1SB18	LABI1-SB18	LABI1-SB18 is an 18” passive subwoofer, 500W AES 8Ω, designed for fixed installations and portable	1 608,40 €
applications (external amplification required). A stand alone compact subwoofer or combined with LABI1-C100i to create a complete powerful solution, easy to mount and plug and play. Dimensions: 513 x 513 x 704 mm / 20.2" x 20.2" x 27.7". Weight: 37kg / 81.8 lb.
	2 042,66 €
	651 400 Ft
	827 278 Ft



	CLABI1SB18P	LABI1-SB18p	LABI1-SB18p is an 18” powered subwoofer, designed for fixed installations and portable applications. A  3 249,63 €
stand alone compact subwoofer or combined with LABI1-C100i to create a complete solution. It performs 2400W Class D built-in amplification power: 1 x 1200W for its low frequency woofer, and 2x600W amplifiers, able to power up to 4 x LABI1-C100i. It also features DC protection to avoid damage to the loudspeakers, and performs 18 factory presets - selectable through the LCD screen. Dimensions: 513 x 513 x 704 mm / 20.2" x 20.2" x 27.7". Weight: 37kg / 81.8 lb.
	4 127,03 €
	1 316 100 Ft
	1 671 447 Ft


Ref.
Name
LABI1 PACKS
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CLABI1PACK1	LABI1PACK1	14 672,59 €
2 x LABI1-SB18p
4 x LABI1-C100i
2 x LABI1-SAC
2 x LABI1-CAC
2 x LABI1-SPC
2 x LABI1-CFC
2 x LABI1-SWK
	18 634,19 €
	5 942 400 Ft
	7 546 848 Ft



	CLABI1PACK2	LABI1PACK2	7 335,80 €
1 x LABI1-SB18p
2 x LABI1-C100i
1 x LABI1-SAC
1 x LABI1-CAC
1 x LABI1-SPC
1 x LABI1-CFC
1 x LABI1-SWK
	9 316,47 €
	2 971 000 Ft
	3 773 170 Ft



	CLABI1PACK3	LABIPACK3	12 150,37 €
2 x LABI1-SB18p
4 x LABI1-C100i
2 x LABI1-SAC
2 x LABI1-CAC
	15 430,97 €
	4 920 900 Ft
	6 249 543 Ft




	CLABI1PACK4
	LABIPACK4
2 x LABI1-SB18p
2 x LABI1-C100i
2 x LABI1-SAC
	
+
	
+ + +	+
	9 128,64 €
	11 593,38 €
	3 697 100 Ft
	4 695 317 Ft


INDUSTRIAL LOUDPEAKERS



	CERK108	eRK108	Outdoor and cost-effective ground loudspeaker. It features a 8" woofer, 0.5" tweeter. 70/100V	176,79 €
transformer (15W). IP65 rated. Ready to be installed in gardens, theme parks, leisure facilities, etc. Dimensions 325x290x270mm. Weight 5kg
	224,52 €
	71 600 Ft
	90 932 Ft




	CECS803	eCS803	Column loudspeaker, featuring 8 x 3" woofer transducers, 100 WRMS @ 8Ω, low impedance direct	167,65 €
connection and 70/100V transformer (Selector de potencia: 30/ 20/ 10/ 5 W 100V/ 8 Ω). Aluminium enclosure with included wall bracket and IP44 outdoor class. Dimensions (without accessories) 105x760x90mm. Weight 4.5 kg
	212,92 €
	67 900 Ft
	86 233 Ft




	CEPRS10TI	ePRS10Ti	10 WRMS sound projector carefully selected for the most extended 70/100V paging and background	81,48 €
music applications. Manufactured in reinforced ABS and IP55 rated, therefore suitable for outdoor superior performance in music high-quality applications.
Power selection: 2,5/5/10W @ 100V. Dimensions Ø 138 x 205mm. Weight 1.6kg (including accessories).
	103,48 €
	33 000 Ft
	41 910 Ft



	CEPRS20TI	ePRS20Ti	20 WRMS sound projector carefully selected for the most extended 70/100V paging and background	86,42 €
music applications. Manufactured in reinforced ABS and IP55 rated, therefore suitable for outdoor superior performance in music high-quality applications. Power selection: 5/ 10/ 20W @ 100V. Dimensions Ø 170 x 245mm. Weight 1.8 kg (including accessories).
	109,75 €
	35 000 Ft
	44 450 Ft



	CEPHS30TI	ePHS30Ti	30 WRMS horn loudspeaker carefully selected for the most extended 70/100V paging and background	109,38 €
music applications, offering durability and optimal speech and music reproduction. Manufactured in reinforced ABS and IP66 rated, therefore suitable for outdoor superior performance.
Power selection: 30W / 20W / 10W / 5W @ 100V. 30WRMS @ 8Ω. Dimensions Ø 246 x 292mm. Weight 2.4kg (including accessories).
	138,92 €
	44 300 Ft
	56 261 Ft



	CEMSP50TI	eMSP50Ti	50 WRMS 2-way musical horn carefully selected for the most extended 70/100V paging and	226,91 €
background music applications, offering durability and optimal speech and music reproduction. Manufactured in reinforced ABS and IP66 rated, therefore suitable for outdoor superior performance in music high-quality applications.
Power selection:2.6/4.5/9/12.5/25/50W @ 100V. 50WRMS @8Ω. Dimensions 362x252x310mm. Weight 3.9kg (including accessories).
	288,18 €
	91 900 Ft
	116 713 Ft



	REMOTE CONTROLS & INTERFACES	EUR	ár EUR	HUF	HUF
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
MPAGE SERIES
Name
Ref.
Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF
Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF
REF.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	PAGING STATIONS	


	CPAGENETDN	PAGENETDN	Desktop paging console for voice notices with Dante™ audio over IP. Features a 10” touch screen, a	2 302,47 €
server client and a UCP server (User Control Panel). Since it’s a server/UCP client device, it’s possible to add other kind of control panels beside the ones destined for voice messages such as: volume control, sound source selection, presets recovery, communication via TCP/UDP with external devices, etc.
Power over Ethernet or local power supply. Gooseneck microphone included.
	2 924,14 €
	932 500 Ft
	1 184 275 Ft



	CEMPAGE	eMPAGE	Digital paging station (MPAGE16’s evolution), compatible with HUB, MIMO88, MIMO88SG and	620,25 €
MIMO1212SG digital matrixes. Includes: a gooseneck cardioid microphone (removable); 16 zone- selection keys; ALL, CLEAR and PAGE keys; 2 programmable keys, F1 & F2, for zone-group selection. Text labelling for destination areas by means of programmable electronic ink display. Dimensions (microphone excluded) 150mm x 180mm x 50mm. Weight 900g.
	787,71 €
	251 200 Ft
	319 024 Ft





	CMPAGE1R	MPAGE1r	1-zone desktop paging station, compatible with any device including a phantom-powered microphone	212,84 €
input (SAM series, COMPACT series, DAM614, MIMO88, CA series, HMA series, etc.). Internal connections for a secure wiring. Dimensions (microphone excluded) 120mm x 126mm x 43mm. Weight 625 g.
	270,31 €
	86 200 Ft
	109 474 Ft



	CMPAGE4	MPAGE4	4-zone desktop paging station compatible with DAM614, CA series, etc. It allows for real-time paging	344,20 €
with zones' destination selection. Selectable chime melody. Dimensions (microphone excluded) 120mm x 126mm x 43mm. Weight 650 g.
	437,13 €
	139 400 Ft
	177 038 Ft



	DIGITAL CONTROLS & PANELS	
Ref.
Name
PULSO Series
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	NEW!
	CPULSO4
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	PULSO-4
	PULSO-4 is a digital remote wall panel with an elegant minimalistic design. Featuring aluminum frame and capacitive 4" TFT 480x480 display, the new PULSO wall panels are the perfect choice to load the User Control Panels of VIDA Series, EclerNet and HUB Series. Single unit EU electrical wall box. PoE or external power supply.
	500,74 €
	635,94 €
	202 800 Ft
	257 556 Ft



	NEW!
	CPULSO6
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	PULSO-6
	PULSO-6 is a digital remote wall panel with an elegant minimalistic design. Featuring aluminum frame and capacitive 5,5" TFT 720x1280 display, the new PULSO wall panels are the perfect choice to load the User Control Panels of VIDA Series, EclerNet and HUB Series. Single unit EU electrical wall box. PoE or external power supply.
	651,11 €
	826,91 €
	263 700 Ft
	334 899 Ft



	NEW!
	CPULSO10
	PULSO-10
	PULSO-10 is a digital remote wall panel with an elegant minimalistic design. Featuring aluminum frame and capacitive 10" TFT 1280x 800 display, the new PULSO wall panels are the perfect choice to load the User Control Panels of VIDA Series, EclerNet and HUB Series. Single unit EU electrical wall box. PoE or external power supply.
	1 002,47 €
	1 273,14 €
	406 000 Ft
	515 620 Ft


Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CWPNETTOUCH	WPNETTOUCH	Remote control TFT touchscreen compatible with all EclerNet products such as: MIMO4040DN,	1 094,57 €
MIMO88/SG, MIMO1212SG, and DUO-NET PLAYER. Incorporates a capacitive 10” touch screen, a server client and UCP server (User Control Panel). When including a WPNETTOUCH in an EclerNet installation is not necessary to use a computer to manage connected devices, neither to have the UCP panels created for the project. Power over Ethernet or local power supply. Surface-mount accessories included. Compatible with VESA75 mounting standard.
260x178x28mm, 700gr.
	1 390,10 €
	443 300 Ft
	562 991 Ft



	CWP22DN	WP22DN	Dante™ interface in a wall panel format. It features 2 audio MIC/LINE Combo connector inputs in its	767,65 €
frontal panel and 2 Dante™ conversion channels either directly or by the sum of channels (stereo to mono conversion). Also, it features 2 analogue outputs with duplicated connectors in XLR format for the front panel and Euroblock on the rear panel, both linked to 2 Dante™ channels coming from the local network. PoE supply or local power supply.
	974,92 €
	310 900 Ft
	394 843 Ft



	CWPNET4KVR	WPNET4KV	EclerNet compatible wall panel. It features a LCD screen, encoder and 4 selection keys. Works perfectly	404,44 €
to enable volume control, source and preset selection functions. Ethernet interface. PoE or local power supply.
	513,64 €
	163 800 Ft
	208 026 Ft



	CWPNET8KR	WPNET8K	EclerNet compatible wall panel. It features a LCD screen and 8 selection keys. Works perfectly to enable	404,44 €
presets or source selection functions. Ethernet interface. PoE or local power supply.
	513,64 €
	163 800 Ft
	208 026 Ft



	CEMCONTROL1R	eMCONTROL1	Digital control panel for the HUB matrix with a wall format, It makes it possible to act as a zone	199,75 €
control, enabling the user to have 3 functions : volumen adjustment/MUTE, selection of musical sources and EQ adjustment with 3 band tone control. Coupled to a WPa type panel with an audio connector, provide remote control + balanced audio signal to the HUB, using only a single CAT5 type cable or higher. Universal surface-mount installation box included. Dimensions 86 x 38 x 86 mm.
	253,69 €
	80 900 Ft
	102 743 Ft



	CEMCTROL1US	eMCTROL1US	Digital control panel for the HUB matrix with a wall format with USA frame. It makes it possible to act	199,75 €
as a zone control, enabling the user to have 3 functions : volumen adjustment/MUTE, selection of musical sources and EQ adjustment with 3 band tone control. Coupled to a WPa type panel with an audio connector, provide remote control + balanced audio signal to the HUB, using only a single CAT5 type cable or higher. Dimensions 116.5x114.8x27mm
	253,69 €
	80 900 Ft
	102 743 Ft





	ANALOGUE CONTROLS & PANELS	
Ref.
Name
WPa SERIES
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF



	CWPABT	WPaBT	Class 1 bluetooth receiver (range 25m) A2DP profile, which keeps the standard wall-panel format of the	247,90 €
WPa series. Include a Euroblock balanced stereo output, double-mono configurable. Easy device name, PIN, stereo / mono output configuration using the Ecler Bluetooth® Manager application for Windows devices. GPO available, useful for automatic priority management. Surface installation box included. Dimensions 86 x 38 x 86 mm.
	314,83 €
	100 400 Ft
	127 508 Ft



	CWPAMIXT	WPaMIX-T	2 channel micro-mixer which keeps the standard wall-panel format of the WPm series. It allows to a	142,47 €
mix a stereo unbalanced signal (2xRCA) with a microphone signal (XLR), getting a balanced mono output that can be sent to a preamplifier, amplifier, mixer, digital or analogue matrix, etc.
The MIC input includes a 2 band EQ (BASS, TREBLE) and talk-over function. Universal surface-mount installation box included. Dimensions 86 x 38 x 86 mm.
	180,94 €
	57 700 Ft
	73 279 Ft



	CWPAMIXTUS	WPaMIX-TUS	2 channel micro-mixer which keeps the standard wall-panel format of the WPm series, but with USA	142,47 €
frame. It allows to a mix a stereo unbalanced signal (2xRCA) with a microphone signal (XLR), getting a balanced mono output that can be sent to a preamplifier, amplifier, mixer, digital or analogue matrix, etc.
The MIC input includes a 2 band EQ (BASS, TREBLE) and talk-over function. Dimensions 116.5x114.8x27mm
	180,94 €
	57 700 Ft
	73 279 Ft



	CWPAVOL	WPaVOL	Remote wall panel control for one volume management. Compatible with all Ecler 0-10V DC REMOTE	77,28 €
control port, like ALMA, MIMO88 / SG, NXA series, CA series, GPA series, etc. Universal surface-mount installation box included. Dimensions 86 x 38 x 86 mm.
	98,15 €
	31 300 Ft
	39 751 Ft



	CWPAVOLUS	WPaVOLUS	Remote wall panel control with USA frame for one volume management. Compatible with all Ecler 0-	89,38 €
10V DC REMOTE control port, like MPA-R, ALMA, MIMO88 / SG, NXA series, CA series, GPA series, etc. Dimensions 116.5x114.8x27mm
	113,52 €
	36 200 Ft
	45 974 Ft



	CWPAVOLJ	WPaVOL-J	Remote wall panel control for one volume management and a front panel stereo mini-jack connector.	90,37 €
Compatible with all ECLER 0-10V DC REMOTE control port, like MPA-R, ALMA, MIMO88 / SG, NXA series, CA series, GPA series, etc.
	114,77 €
	36 600 Ft
	46 482 Ft



	CWPAVOLSR	WPaVOL-SR	Remote wall panel control for one volume management + source or preset selection. Compatible with	110,37 €
all Ecler 0-10V DC REMOTE control port, like MPA-R, ALMA, MIMO88 / SG, NXA series, CA series, GPA series, etc.
Universal surface-mount installation box included. Dimensions 86 x 38 x 86 mm.
	140,17 €
	44 700 Ft
	56 769 Ft



	CWPAVOLSRUS	WPaVOL-SRUS	Remote wall panel control with USA frame for one volume management + source or preset selection.	110,37 €
Compatible with all Ecler 0-10V DC REMOTE control port, like MPA-R, ALMA, MIMO88 / SG, NXA series, CA series, GPA series, etc.
Dimensions 116.5x114.8x27mm
	140,17 €
	44 700 Ft
	56 769 Ft



	CWPAVOLSRJ	WPaVOL-SR-J	Same features as WPaVOL-SR + front panel stereo mini-jack connector.	115,56 €
Universal surface-mount installation box included. Dimensions 86 x 38 x 86 mm.
	146,76 €
	46 800 Ft
	59 436 Ft



	CWPACNXCBO	WPaCNX-CBO	Connection wall plate with Female 3 pin XLR connector + Jackk ST (combo connector). Screw-type	86,42 €
connector at the back (no solder needed).
Universal surface-mount installation box included. Dimensions 86 x 38 x 86 mm.
	109,75 €
	35 000 Ft
	44 450 Ft



	CWPACNXJRCA	WPaCNX-JRCA	Connection wall plate with 1 x stereo minijack and 2 x RCA connectors.	81,48 €
Universal surface-mount installation box included. Dimensions 86 x 38 x 86 mm.
	103,48 €
	33 000 Ft
	41 910 Ft



	CWPAHAT6	WPaH-AT6	70 / 100V line attenuator with integrated 24 VDC priority relay. 6W maximum output power.	94,32 €
Universal surface-mount installation box included. Dimensions 86 x 38 x 86 mm.
	119,79 €
	38 200 Ft
	48 514 Ft



	CWPAHAT40	WPaH-AT40	70 / 100V line attenuator with integrated 24 VDC priority relay. 40W maximum output power.	113,58 €
Universal surface-mount installation box included. Dimensions 86 x 38 x 86 mm.
	144,25 €
	46 000 Ft
	58 420 Ft



	CWPAHAT100	WPaH-AT100	70 / 100V line attenuator with integrated 24 VDC priority relay. 100W maximum output power.	121,48 €
Universal surface-mount installation box included. Dimensions 172 x 38 x 86 mm.
	154,28 €
	49 200 Ft
	62 484 Ft





	CUBWPAVOL	UBWPaVOL	UBWPaVOL is a remote wall panel control for one volume management, in US single gang bare format.	81,48 €
It is compatible with Ecler devices including 0-10VDC or 0-12VDC remote control ports (internal jumper selectable). Dimensions: 35x65x35mm / 1.4"x2.5"x1.4". Weight: 30gr / 0.07 lb.
	103,48 €
	33 000 Ft
	41 910 Ft



	CUBWPACNXJRC	UBWPaCNXJRC	UBWPaCNX-JRC is a connection wall-panel, in US single gang bare format, with 1 x stereo minijack and	76,30 €
2 x RCA connectors. This connector can be screwed at the rear (does not require any soldering). Dimensions: 35x65x35mm / 1.4"x2.5"x1.4". Weight: 30gr / 0.07 lb.
	96,90 €
	30 900 Ft
	39 243 Ft



	ACCESSORIES	

	PRODUCT ACCESSORIES	
Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CETH232AD	ETH232AD	Ecler ETH232AD is a serial interface that allows bidirectional transparent transmission between RS-	219,75 €
232/422/485 and Ethernet. It includes a setting webpage for Ethernet and Serial customized settings. Dimensions: 100 × 86 × 26 mm (3.94” × 3.39” × 1.02”) Weight: 0.5kg / 1.10 lb.
	279,09 €
	89 000 Ft
	113 030 Ft



	C1UHRMKIT	1UHRMKIT	Kit that enables a half-width x 1U height rack device to be mounted into a standard width rack cabinet.	28,15 €
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	35,75 €
	11 400 Ft
	14 478 Ft



	C2UHRMKIT	2UHRMKIT	Kit that enables a half-width x 2U height rack device to be mounted into a standard width rack cabinet.	37,28 €
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	47,35 €
	15 100 Ft
	19 177 Ft



	CVEORACK19	VEORACK19	Universal 19" rack mount accessory. Mounting screws and Velkro® included.	101,48 €
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	128,88 €
	41 100 Ft
	52 197 Ft



	CPUM3	PUM3	Ecler PUM3 is a rack-mount accessory that allows to mount two half-width RU devices in 1 standard	18,27 €
width RU space. Mounting screws included.
	23,20 €
	7 400 Ft
	9 398 Ft



	CWPA2FMBOX	WPa2FMBOX	Double Flush-Mount box, compatible with the WPa wall panel series. It includes a single frame for	52,35 €
fitting 2 adjacent panels in a twin housing.
	66,48 €
	21 200 Ft
	26 924 Ft



	CWPA2SMBOX	WPa2SMBOX	Double Surface-mount box, compatible with the WPa wall panel series. It includes a single frame for	52,35 €
fitting 2 adjacent panels in a twin housing.
	66,48 €
	21 200 Ft
	26 924 Ft



	CWP24PSU	WP24-PSU	Ecler WP24-PSU is a 24VDC 0.5A external PSU. International AC plugs set. Coaxial connector (+ center),	49,38 €
compatible with eMPAGE, DN44BOB, WPNET Series, eMCONTROL1, WPaMIX-T and WPaBT.
	62,72 €
	20 000 Ft
	25 400 Ft



	CLABI1SWK	LABI1-SWK	Subwoofer-Wheel-Kit. 4 wheel kit for LABI1-SB18/18p subwoofer	159,75 €
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	202,89 €
	64 700 Ft
	82 169 Ft



	CLABI1CFC	LABI1-CFC	Column-Flight-Case. Flight case for 2 LABI1-C100i + wiring + mounting accessories	972,35 €
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	1 234,88 €
	393 800 Ft
	500 126 Ft





	CLABI1SPC	LABI1-SPC	Subwoofer-Protection-Cover. Nylon protection cover for LABI1-SB18/18p subwoofer	196,79 €
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	249,92 €
	79 700 Ft
	101 219 Ft



	AUDIO CABLES & OTHERS	
Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CMBSTAND	MBSTAND	Microphone floor boom stand.	57,28 €
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	72,75 €
	23 200 Ft
	29 464 Ft



	CMDSTAND	MDSTAND	Microphone desktop stand.	15,06 €
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	19,13 €
	6 100 Ft
	7 747 Ft



	CNXAC8RM	CNXAC8RM	8 x Schuko sockets rack mount AC strip + ON/OFF switch, 1 RU.	43,21 €
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	54,88 €
	17 500 Ft
	22 225 Ft



	CNXEBEB1	CNXEBEB1	Euroblock 3 pin to Euroblock 3 pin premade cable, 1 metre length.	22,22 €
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	28,22 €
	9 000 Ft
	11 430 Ft



	CNXEBEB2M5	CNXEBEB2M5	Euroblock 3 pin to Euroblock 3 pin premade cable, 2.5 metre length.	23,21 €
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	29,48 €
	9 400 Ft
	11 938 Ft



	CNXEBLINK4	CNXEBLINK4	Euroblock 3 pin to Euroblock 3 pin, 4 connectors premade link cable (amplifiers, preamps and mixers	22,22 €
inputs link wire, to share the same audio signal).
	28,22 €
	9 000 Ft
	11 430 Ft



	CNXEBRCA1	CNXEBRCA1	Double Euroblock 3 pin to double RCA male and female connection premade cable including RCA to	26,17 €
Euroblock unbalancing, 1 metre length.
	33,24 €
	10 600 Ft
	13 462 Ft



	CNXRCAEBAD	CNXRCAEBAD	Euroblock 3 pin to RCA MONO female adapter including RCA to Euroblock unbalancing.	19,26 €
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	24,46 €
	7 800 Ft
	9 906 Ft



	CNXMJXLR2	CNXMJXLR2	2m lenght minijack ST to mono XLR male. Includes an internal resistance for overload protection and a	26,17 €
propper sum of the signals.
	33,24 €
	10 600 Ft
	13 462 Ft



	CNXXLRFEB	CNXXLRFEB	Euroblock 3 pin to XLR female connection premade cable, 0.5 metre length.	17,28 €
[image: ]

	21,95 €
	7 000 Ft
	8 890 Ft



	CNXXLRXLR1	CNXXLRXLR1	XLR male to XLR female cable, 1 metre length.	19,26 €
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	24,46 €
	7 800 Ft
	9 906 Ft



	CNXXLRXLR5	CNXXLRXLR5	XLR male to XLR female cable, 5 metre length.	36,30 €
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	46,10 €
	14 700 Ft
	18 669 Ft



	CNXXLRXLR10	CNXXLRXLR10	XLR male to XLR female cable, 10 metre length.	56,30 €
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	71,50 €
	22 800 Ft
	28 956 Ft



	LOUDSPEAKERS HARDWARE	
Ref.
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CFLATYBK	FLATY	FLATY is a wall bracket that allows the columns of the MIA series to be installed attached to the wall. It	30,12 €
is made of stainless steel and allows the height to be adjusted at any point along the length of the column, as well as allowing 2 columns to be installed side by side on top of each other. Black color.
	38,26 €
	12 200 Ft
	15 494 Ft



	CFLATYWH	FLATY	FLATY is a wall bracket that allows the columns of the MIA series to be installed attached to the wall. It	30,12 €
is made of stainless steel and allows the height to be adjusted at any point along the length of the column, as well as allowing 2 columns to be installed side by side on top of each other. White color.
	38,26 €
	12 200 Ft
	15 494 Ft



	CHANDYBK	HANDY	HANDY is a wall bracket compatible with the MIA and NIMBO-14 series. It is incredibly versatile and	51,36 €
intelligent with swivel and tilt adjustment, made of stainless steel. Black color.
	65,22 €
	20 800 Ft
	26 416 Ft



	CHANDYWH	HANDY	HANDY is a wall bracket compatible with the MIA and NIMBO-14 series. It is incredibly versatile and	51,36 €
intelligent with swivel and tilt adjustment, made of stainless steel. White colour.
	65,22 €
	20 800 Ft
	26 416 Ft



	CGROUNDYBK	GROUNDY	GROUNDY is a bracket that allows you to install eMOTUS series speakers on the floor. Compatible with	37,28 €
eMOTUS3OD, eMOTUS5P, eMOTUS5PB and eMOTUS5OD. Available in black colour.
	47,35 €
	15 100 Ft
	19 177 Ft



	CCEILYBK	CEILY	CEILY is a bracket that allows eMOTUS series speakers to be mounted on the ceiling. Compatible with	41,23 €
eMOTUS3OD, eMOTUS5P, eMOTUS5PB and eMOTUS5OD. Black colour.
	52,37 €
	16 700 Ft
	21 209 Ft



	CCEILYWH	CEILY	CEILY is a bracket that allows eMOTUS series speakers to be mounted on the ceiling. Compatible with	41,23 €
eMOTUS3OD, eMOTUS5P, eMOTUS5PB and eMOTUS5OD. White colour.
	52,37 €
	16 700 Ft
	21 209 Ft



	CRAILAPTORWH	RAILAPTOR	RAILAPTOR is an adapter for hanging compatible loudspeakers from a ceiling light rail. It is suitable for	25,19 €
eMOTUS5OD, AUDEO103 and AUDEO106 cabinets and light rails performing 4 wire 3 circuit track system such as Global Track Pro, Eutrac or other compatible systems. Dimensions: 85x150x30 mm / 3.3"x5.9"x1.2". Weight: 130gr / 0,29lb. White colour.
	31,99 €
	10 200 Ft
	12 954 Ft



	CRAILAPTORBK	RAILAPTOR	RAILAPTOR is an adapter for hanging compatible loudspeakers from a ceiling light rail. It is suitable for	25,19 €
eMOTUS5OD, AUDEO103 and AUDEO106 cabinets and light rails performing 4 wire 3 circuit track system such as Global Track Pro, Eutrac or other compatible systems.
	31,99 €
	10 200 Ft
	12 954 Ft



	CARQ108UBBK	ARQ108UBBK	Optional U-BRACKET accessory kit available for the ARQIS108i model.	47,16 €
Black colour.
	59,89 €
	19 100 Ft
	24 257 Ft



	CARQ108UBWH	ARQ108UBWH	Optional U-BRACKET accessory kit available for the ARQIS108i model.	47,16 €
White colour.
	59,89 €
	19 100 Ft
	24 257 Ft



	CARQ110UBBK	ARQ110UBBK	Optional U-BRACKET accessory kit available for the ARQIS110i model.	58,27 €
Black colour.
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	74,00 €
	23 600 Ft
	29 972 Ft



	CARQ110UBWH	ARQ110UBWH	Optional U-BRACKET accessory kit available for the ARQIS110i model.	58,27 €
White colour.
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	74,00 €
	23 600 Ft
	29 972 Ft



	CARQ112UBBK	ARQ112UBBK	Optional U-BRACKET accessory kit available for the ARQIS112i model.	63,21 €
Black colour.
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	80,28 €
	25 600 Ft
	32 512 Ft





	CARQ112UBWH	ARQ112UBWH	Optional U-BRACKET accessory kit available for the ARQIS112i model.	63,21 €
White colour.
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	80,28 €
	25 600 Ft
	32 512 Ft



	EOL
	CARQSB10SATB
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	ARQSB10SATB
	Kit including 2 metal brackets, to convert an ARQISSB10i subwoofer unit into a hanging cluster, combining the ARQIS SB10 unit and 4 x eAMBIT103 satellite loudspeakers.
(loudspeakers not included with this reference)
	90,37 €
	114,77 €
	36 600 Ft
	46 482 Ft



	EOL
	CAVICCAN6L
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	AVICCAN6L
	Low Profile Back Can for VIC6 in-ceiling loudspeakers. Delivered by master carton of 2 units. Price per unit.
	40,25 €
	51,11 €
	16 300 Ft
	20 701 Ft



	CAVICSG	AVICSG	Printable squared grill for VIC series (6 & 8 inches compatible).	48,40 €
Magnetic fixation. White colour.
Delivered by master carton of 2 units. Price per pair.
	61,46 €
	19 600 Ft
	24 892 Ft



	CAVICRG6BK	AVICRG6	Printable round grill for VIC series (6 inches compatible).	38,27 €
Magnetic fixation. Black colour.
Delivered by master carton of 2 units. Price per pair.
	48,60 €
	15 500 Ft
	19 685 Ft



	CAVICRG6WH	AVICRG6	Printable round grill for VIC series (6 inches compatible).	36,30 €
Magnetic fixation. White colour.
Delivered by master carton of 2 units. Price per pair.
	46,10 €
	14 700 Ft
	18 669 Ft



	CAVICRG8BK	AVICRG8	Printable round grill for VIC series (8 inches compatible).	36,30 €
Magnetic fixation. Black colour.
Delivered by master carton of 2 units. Price per pair.
	46,10 €
	14 700 Ft
	18 669 Ft



	CAVICRG8WH	AVICRG8	Printable round grill for VIC series (8 inches compatible).	40,25 €
Magnetic fixation. White colour.
Delivered by master carton of 2 units. Price per pair.
	51,11 €
	16 300 Ft
	20 701 Ft



	CICTB6	IC-TB6	Tile bridge compatible with IC6 in-ceiling loudspeakers.	40,25 €
Sold in kits of 2 units. Price per kit.
	51,11 €
	16 300 Ft
	20 701 Ft



	CICTB8	IC-TB8	Tile bridge compatible with IC8 and IC6CLASS series in-ceiling loudspeakers.	80,49 €
Sold in kits of 2 units. Price per kit.
	102,23 €
	32 600 Ft
	41 402 Ft



	CCOLORPAINT	COLORPAINT	Launching of painting in ceiling loudspeakers grilles (PKIC6,PKIC8, AVICSG, AVICRG) in a RAL colour .	86,42 €
There is no charge for launching when painting a minimum of 100 units in the same RAL colour.
	109,75 €
	35 000 Ft
	44 450 Ft



	CPAINT1S	PAINT1S	Painting by unit when there are less than 10 units.	240,00 €
	304,80 €
	97 200 Ft
	123 444 Ft



	CPAINT10S	PAINT10S	Painting by unit when there are more than 10 units and with a maximum of 99 units.	39,26 €
	49,86 €
	15 900 Ft
	20 193 Ft



	CPAINT100S	PAINT100S	Painting by unit when there are 100 or more units.	20,25 €
	25,71 €
	8 200 Ft
	10 414 Ft



	CPKIC6	PKIC6	Accessory for personalizing the IC6 ceiling loudspeaker. The kit includes a grille that can be painted	14,07 €
(with the appearance of the IC6CLASS) and an accessory (anchor ring) to mount this grille on the IC6. Easy to paint and mount.
	17,87 €
	5 700 Ft
	7 239 Ft





	CPKIC8	PKIC8	Accessory to personalize the IC8 ceiling loudspeaker. The kit includes a grille that can be painted (with	42,22 €
the appearance of the IC6CLASS) and an accessory (anchor ring) to mount this grill on the IC8. Easy to paint and mount.
	53,62 €
	17 100 Ft
	21 717 Ft



	CPOLE01	POLE01	Adjustable 35 mm rod for pole for loudspeaker mount on top of a sub-woofer unit (ARQIS110i on top	42,22 €
of ARQISSB15).
	53,62 €
	17 100 Ft
	21 717 Ft



	CSR12	SR12	Mount bracket for ARQIS110i and ARQIS112i loudspeakers.	38,27 €
Delivered by master carton of 2 units. Price per unit.
	48,60 €
	15 500 Ft
	19 685 Ft



	CTRIPO1	TRIPO1	Loudspeaker floor stand with 35 MM pole.	75,31 €
Delivered by master carton of 2 units. Price per unit.
	95,64 €
	30 500 Ft
	38 735 Ft



	CLABI1SAC	LABI1-SAC	Subwoofer-adapter-column, to install the LABI1-C100i satellite loudspeaker on LABI1-SB18p	180,74 €
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	229,54 €
	73 200 Ft
	92 964 Ft



	CLABI1CAC	LABI1-CAC	Column-adapter-column, to connect vertically two LABI1-C100i column loudspeakers. Includes 60cm	215,80 €
Speakon®-Speakon® cable.
Warning: Only for stacking, NOT for flying
	274,07 €
	87 400 Ft
	110 998 Ft



	CLABI1TBC	LABI1-TBC	Truss-Bracket-Column. Support to install a LABI1-C100i loudspeaker to truss	130,62 €
[image: ]

	165,88 €
	52 900 Ft
	67 183 Ft



	CLABI1PBC	LABI1-PBC	Pole-Bracket-Column. Pole adaptor to install LABI1-C100i loudspeakers in a 35mm standard pole	221,73 €
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	281,60 €
	89 800 Ft
	114 046 Ft



	CLABI1WBC	LABI1-WBC	Wall-Bracket-Column. LABI1-C100i wall mount bracket	147,65 €

[image: ]

	187,52 €
	59 800 Ft
	75 946 Ft



	CLABI1HBC	LABI1-HBC	Horizontal-Bracket-Column. High-density foam pieces to let LABI1-C100i rest on the floor horizontally.	37,28 €
Allows 0º/ 30º/ 45º inclinations relative to the horizontal surface
	47,35 €
	15 100 Ft
	19 177 Ft



	CLABI1ODCNX	LABI1-ODCNX	Outdoor kit to cover LABI1-C100i connections and make it ready for outdoor applications	75,31 €
[image: ]

	95,64 €
	30 500 Ft
	38 735 Ft





VIDEO


	SWITCHERS	
Ref
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF




	CVEOSWC44	VEO-SWC44	Wireless conferencing and presentation switcher with Full HD video resolution wireless inputs and a 4K	972,35 €
/ UHD HDMI 2.0 video output. It supports wireless connection for USB devices like webcam and mic via dongle, Windows & macOS applications and is also Airplay / Miracast compliant. An integrated audio de-embedder provides stereo unbalanced analogue output on a 3,5mm jack connector. Includes a WebGUI for configuration and management as well as RS-232,TCP/IP remote control, all enabled by a pair of LAN RJ-45 connectors with independent networks available. Support for PoE. Dimensions 41x220x120 mm / 1.6"x8.66"x4.72". Weight 1 kg / 2.2 lb.
	1 234,88 €
	393 800 Ft
	500 126 Ft



	CVEOSWC44TU	VEO-SWC44TU	Plug-n-play USB Type-C for VEO-SWC44 wireless connection with a laptop or PC.	303,21 €
	385,08 €
	122 800 Ft
	155 956 Ft



	CVEOSWC44TH	VEO-SWC44TH	Plug-n-play HDMI for VEO-SWC44 wireless connection with a laptop or PC.	303,21 €

[image: ]

	385,08 €
	122 800 Ft
	155 956 Ft



	NEW!
	CVEOSWC45
	VEO-SWC45
	VEO-SWC45 is a professional 4K presentation and conferencing switcher designed for seamless connectivity via HDMI and wireless technologies. Supporting effortless collaboration, it features two HDMI video outputs with advanced screen management and a set of USB ports for integration with existing videoconference systems, including smart local camera switching capabilities. 1080p wireless presentation and conferencing are enabled through Chromecast, Miracast, Airplay, VEOShare app, and 4K wireless transmitter accessories VEO-SWC45TH and VEOSWC45TU for HDMI and USB-C connections. Dimensions 41x220x120 mm / 1.6"x8.66"x4.72". Weight 1 kg / 2.2 lb.
	1 303,46 €
	1 655,39 €
	527 900 Ft
	670 433 Ft



	NEW!
	CVEOSWC45TU
	VEO-SWC45TU
	Plug-n-play USB Type-C for VEO-SWC45 wireless connection with a laptop or PC.
	316,05 €
	401,38 €
	128 000 Ft
	162 560 Ft



	NEW!	CVEOSWC45TH	VEO-SWC45TH	Plug-n-play HDMI for VEO-SWC45 wireless connection with a laptop or PC.	316,05 €
	401,38 €
	128 000 Ft
	162 560 Ft



	CVEOSWM44	VEO-SWM44	VEO-SWM44 is a compact 4K presentation switcher that includes 2 HDMI 2.0, a USB-C and	1 258,27 €
Miracast/Airplay wireless input selection via VEOCast to a single HDMI 2.0 output, supporting resolutions up to 4K/60Hz 4:4:4 HDR10 and Dolby Vision. An integrated audio de-embedder provides stereo analogue balanced outputs on Euroblock connectors. VEO-SWM44 includes 2 USB 3.0 type B and 2 USB 3.0 type A in order to support soft codec applications and external devices like webcam and KVM kits. Input selection is available via Auto-switching function, front panel buttons or RS-232.
Display control via front panel buttons through CEC or RS-232. Smart EDID management and HDCP 2.2 support.
Dimensions (WxHxD) 220mm x 44mm x 150mm / 8.66“ x 1.73“ x 5.90“ Weight 1,25 Kg / 2.75 lb
	1 598,00 €
	509 600 Ft
	647 192 Ft



	CVEOSWH44	VEO-SWH44	4x1 HDMI switcher for high dynamic range (HDR) formats. It is HDCP 2.2 compliant and supports	230,86 €
4K/UHD video @ 60 Hz with 4:4:4 chroma sampling, as well as HDMI signals with bandwidth up to 18 Gbps. It is the ideal solution for applications requiring 4K/UHD and HDR sources and displays. VEO- SWH44 includes audio de-embedding features and audio EDID management. The HDMI selection could be automatic (sense selection) and manual (frontal panel, remote control or serial commands). The controls include ARC mute and LED indications of the selected sources and settings.
Dimensions (WxHxD) 85 x 12 x 180 mm / 3.34” x 0.47” x 7.09” Weight 300g / 0.66 lb
	293,20 €
	93 500 Ft
	118 745 Ft





	MATRIXES	
Ref
Name
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF





	CVEOMXH44D	VEO-MXH44D	4x4 HDMI 2.0 matrix with support for up to 4K/UHD video resolution, 60 Hz and	714,32 €
4:4:4 chroma sampling. It includes 8 analogue and digital audio de-embedding outputs as well as EDID management, a LCD display and an integrated WebGUI that allows to configure and control the unit. VEO-MXH44D can load and launch up to 8 presets which makes it a very interesting solution for professional applications that require video and audio HDMI signals routing between 4K/UHD sources and displays with a smart control management. Control via front panel and display, IR remote, RS-232 control, IP control and WebGUI. Dimensions 34x216x128mm / 1,34”x8,50”x5,04”. Weight 470g / 1,04 lb.
	907,19 €
	289 300 Ft
	367 411 Ft



	CVEOMXH88D	VEO-MXH88D	8x8 HDMI 2.0 matrix with support for up to 4K/UHD video resolution, 60 Hz and 4:4:4	2 000,49 €
chroma sampling. It includes 8 analogue audio inputs and 16 analogue and digital audio de-embedding outputs as well as EDID management, a LCD display and an integrated WebGUI that allows to configure and control the unit. VEO-MXH88D can load and
launch up to 8 presets which makes it a very interesting solution for professional applications that require video and audio HDMI signals routing between 4K/UHD sources and displays with a smart control management. Control via front panel and display, IR remote, RS-232 control, IP control and WebGUI. Dimensions 44x482x220mm / 1,73”x18,97”x8,66”. Weight 2800g / 6,17 lb.
	2 540,63 €
	810 200 Ft
	1 028 954 Ft



	NEW!
	CVEOMXH48T
	VEO-MXH48T
	VEO-MXH48T is a 8x8 HDBaseT and HDMI® matrix with support for up to 4K/UHD video resolution, 60 Hz and 4:4:4 chroma sampling. It includes 8 analogue audio inputs and 16 analogue and digital audio de-embedding outputs as well as EDID management, a LCD display and an integrated WebGUI that allows to configure and control the unit in a very user friendly way. The HDBaseT outputs can deliver 4K/UHD video up to 40m and Full HD video up to 70m as well as PoC power supply to HDBaseT compliant receivers. It includes a video downscaler and an independent audio matrix. Dimensions
482.6 x 88 x 394 mm / 19 x 3.46 x 15.51 in. Weight 8.3 Kg / 18.30 lb.
	3 597,78 €
	4 569,18 €
	1 457 100 Ft
	1 850 517 Ft



	SPLITTERS	
Nettó lista ár Bruttó lista  Nettó lista ár  Bruttó lista ár EUR	ár EUR	HUF	HUF


	CVEOSPH42	VEO-SPH42	1×2 HDMI splitter for high dynamic range (HDR) formats. It is HDCP 2.2/1.4 compliant and supports	145,68 €
4K/UHD video @ 60 Hz with 4:4:4 chroma sampling, as well as HDMI signals with bandwidth up to 18 Gbps. It is the ideal solution for applications requiring 4K/UHD and HDR sources and displays. It includes EDID management features, front panel LED indicators for power and signal status.
Dimensions (WxHxD) 94mm x 15mm x 61mm / 3.7“ x 0.59“ x 2.4“ Weight 120g / 0.265 lb
	185,01 €
	59 000 Ft
	74 930 Ft



	CVEOSPH44	VEO-SPH44	1×4 HDMI splitter for high dynamic range (HDR) formats. It is HDCP 2.2/1.4 compliant and supports	189,63 €
4K/UHD video @ 60 Hz with 4:4:4 chroma sampling, as well as HDMI signals with bandwidth up to 18 Gbps. It is the ideal solution for applications requiring 4K/UHD and HDR sources and displays. It includes EDID management features, front panel LED indicators for power and signal status.
Dimensions (WxHxD) 150mm x 17mm x 65mm / 5.9" x 0.67"x 2.56" Weight 245g / 0.54 lb
	240,83 €
	76 800 Ft
	97 536 Ft



	CVEOSPH48	VEO-SPH48	1×8 HDMI splitter for high dynamic range (HDR) formats. It is HDCP 2.2/1.4 compliant and supports	380,25 €
4K/UHD video @ 60 Hz with 4:4:4 chroma sampling, as well as HDMI signals with bandwidth up to 18 Gbps. It is the ideal solution for applications requiring 4K/UHD and HDR sources and displays. It includes EDID management features, front panel LED indicators for power and signal status.
Dimensions (WxHxD) 248mm x 17mm x 110mm / 9.76” x 0.67” x 4.33” Weight 610g / 1.34 lb
	482,91 €
	154 000 Ft
	195 580 Ft



	NEW!
	CVEOSPS42
	VEO-SPS42
	1x2 18Gbps HDMI splitters that allows an HDMI source signal to be distributed and extended to remote displays, supporting up to 4K 60Hz 4:4:4 video signals. It includes an HDMI loop output and two main single Cat outputs, allowing for transmission distances of up to 35 meters for 4K/60Hz, 50 meters for 4K/30Hz, or 60 meters for 1080p over a single Cat 5e or higher cable. Supports one-way IR control signal pass-through, stereo unbalanced audio extraction on Euroblock connector, EDID management, and RS-232 serial control. Dimensions (WxHxD) 94mm x 15mm x 61mm / 3.7“ x 0.59“ x 2.4“ Weight 120g / 0.265 lb
	350,37 €
	444,97 €
	141 900 Ft
	180 213 Ft



	NEW!
	CVEOSPS44
	VEO-SPS44
	1x4 18Gbps HDMI splitters that allows an HDMI source signal to be distributed and extended to remote displays, supporting up to 4K 60Hz 4:4:4 video signals. It includes an HDMI loop output and four main single Cat outputs, allowing for transmission distances of up to 35 meters for 4K/60Hz, 50 meters for 4K/30Hz, or 60 meters for 1080p over a single Cat 5e or higher cable. Supports one-way IR control signal pass-through, stereo unbalanced audio extraction on Euroblock connector, EDID management, and RS-232 serial control. Dimensions (WxHxD) 150mm x 17mm x 65mm / 5.9" x 0.67"x 2.56"
Weight 245g / 0.54 lb
	600,99 €
	763,25 €
	243 400 Ft
	309 118 Ft



	NEW!
	CVEOSPS48
	VEO-SPS48
	1x8 18Gbps HDMI splitters that allows an HDMI source signal to be distributed and extended to remote displays, supporting up to 4K 60Hz 4:4:4 video signals. It includes an HDMI loop output and eight main single Cat outputs, allowing for transmission distances of up to 35 meters for 4K/60Hz, 50 meters for 4K/30Hz, or 60 meters for 1080p over a single Cat 5e or higher cable. Supports one-way IR control signal pass-through, stereo unbalanced audio extraction on Euroblock connector, EDID management, and RS-232 serial control,. Dimensions (WxHxD) 248mm x 17mm x 110mm / 9.76” x 0.67” x 4.33” Weight 610g / 1.34 lb
	1 002,47 €
	1 273,14 €
	406 000 Ft
	515 620 Ft



	VIDEO DISTRIBUTION OVER IP	Nettó lista ár Bruttó lista  Nettó lista ár  Bruttó lista ár EUR	ár EUR	HUF	HUF


	CVEOXTI2L	VEO-XTI2L	VEO-XTI2L and VEO-XRI2L are low latency 4K HDMI extenders over IP. Suitable both for creation of	668,40 €
AVoverIP matrixes in multipoint-tomultipoint configurations and for point-to-point extensions up to 120m via single Cat.5e/6 cable. They also provide optional fiber optic connection for extension of 4K signals up to 2Km. Additional features like analog and digital audio embedding and de-embedding, and videowall option make this product a very versatile solution for many applications. An intuitive user panel with LEDs display allows to select the stream channel just out of the box, without the need of connecting a PC. The extenders can be power supplied both via PoE or via the included external PSU. Web browser interface, PC tools and third party control protocol are available for advanced settings and advanced control.
Dimensions (WxHxD) 170 x 26 x 109 mm / 6.69” x 1.02” x 4.29” Weight 470g / 1.04 lb
	848,86 €
	270 700 Ft
	343 789 Ft



	CVEOXRI2L	VEO-XRI2L	VEO-XTI2L and VEO-XRI2L are low latency 4K HDMI extenders over IP. Suitable both for creation of	740,49 €
AVoverIP matrixes in multipoint-tomultipoint configurations and for point-to-point extensions up to 120m via single Cat.5e/6 cable. They also provide optional fiber optic connection for extension of 4K signals up to 2Km. Additional features like analog and digital audio embedding and de-embedding, and videowall option make this product a very versatile solution for many applications. An intuitive user panel with LEDs display allows to select the stream channel just out of the box, without the need of connecting a PC. The extenders can be power supplied both via PoE or via the included external PSU. Web browser interface, PC tools and third party control protocol are available for advanced settings and advanced control.
Dimensions (WxHxD) 170 x 26 x 109 mm / 6.69” x 1.02” x 4.29” Weight 470g / 1.04 lb
	940,43 €
	299 900 Ft
	380 873 Ft



	CVEOXTI1CG2	VEO-XTI1CG2	VEO-XTI1CG2 transmitter and VEO-XRI1CG2 receiver are a H.265 / H.264 over IP set of extenders that	385,43 €
allow for HDMI distribution over 1Gb Ethernet networks with up to 1080p@60Hz video support. Suitable for various applications which also require PoE, audio management, video wall compositing or RS-232 control, such as educational, commercial or corporate installations, where flexible and scalable AV systems are in need. Signal transmission distance up to 100m over Cat5e/6/7 cable. Support for audio embedding and extraction. Support for pass through and RS-232, TCP/IP, WebGUI management using VEO-XCTRLG2 controller module. Dimensions 21,5x95x120mm
/ 0,85”x3,74”x4,72”. Weight 74g / 0,16 lb.
	489,50 €
	156 100 Ft
	198 247 Ft



	CVEOXRI1CG2	VEO-XRI1CG2	VEO-XTI1CG2 transmitter and VEO-XRI1CG2 receiver are a H.265 / H.264 over IP set of extenders that	385,43 €
allow for HDMI distribution over 1Gb Ethernet networks with up to 1080p@60Hz video support. Suitable for various applications which also require PoE, audio management, video wall compositing or RS-232 control, such as educational, commercial or corporate installations, where flexible and scalable AV systems are in need. Signal transmission distance up to 100m over Cat5e/6/7 cable. Support for audio embedding and extraction. Support for PoE function. Support for pass through and RS-232, TCP/IP, WebGUI management using VEO-XCTRLG2 controller module. Dimensions 21,5x95x120mm / 0,85”x3,74”x4,72”. Weight 74g / 0,16 lb.
	489,50 €
	156 100 Ft
	198 247 Ft



	CVEOXCTRLG2	VEO-XCTRLG2	Control module for and expanded management experience with in-built WEB configuration interface.	360,25 €
Dimensions 204 x 21.5 x 98.5mm / 4.7 x 0.85 x 3.88 in. Weight
0.540 Kg / 1.19 lb
	457,51 €
	145 900 Ft
	185 293 Ft



	NEW!
	CWPTI1CG2
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	WPTI1CG2
	WPTI1CG2 transmitter is a professional H.265 / H.264 device designed for HDMI distribution over 1Gb Ethernet networks, supporting resolutions up to WUXGA and 1080p. It delivers high-quality video compression over distances of up to 100 meters using a single Cat 5e or higher cable. Its wallplate design, featuring an HDMI input, RJ-45 port with PoE, and a reset button, provides an elegant solution for visible installations. Control and configuration are managed via the built-in Web GUI or pairing it with the VEO-XCTRLG2 controller, ensuring an easy setup and reliable performance.. Dimensions 86 x 38 x 86 mm. Weight TBC
	321,23 €
	407,97 €
	130 100 Ft
	165 227 Ft



	EXTENDERS	
Nettó lista ár Bruttó lista  Nettó lista ár  Bruttó lista ár EUR	ár EUR	HUF	HUF


	NEW!
	CVEOXTI4D
	VEO-XTI4D
	VEO-XTI4D transmitter is a professional JPEG2000 over IP extender that enable secure HDMI distribution with 18Gbps bandwidth, supporting 4K 60Hz 4:4:4 video over 1Gb Ethernet networks, reaching distances up to 100 meters on a single Cat 5e or higher cable and a transmission latency of 1- 2 frames. Equipped with dual RJ-45 ports, these units support independent or combined network configurations for Dante AV-A. Advanced video wall management up to a 9x9 configuration is also supported when paired with the VEO-XCTRL4D controller, along with additional control options.
Dimensions: 204 x 25.5 x 136 mm / 8.03 x 1.0 x 5.35 in. Weight: 0.631 Kg / 1.391 lb.
	901,98 €
	1 145,51 €
	365 300 Ft
	463 931 Ft



	NEW!
	CVEOXRI4D
	VEO-XRI4D
	VEO-XTI4D receiver is a professional JPEG2000 over IP extender that enable secure HDMI distribution with 18Gbps bandwidth, supporting 4K 60Hz 4:4:4 video over 1Gb Ethernet networks, reaching distances up to 100 meters on a single Cat 5e or higher cable and a transmission latency of 1-2 frames. Equipped with dual RJ-45 ports, these units support independent or combined network configurations for Dante AV-A. Advanced video wall management up to a 9x9 configuration is also supported when paired with the VEO-XCTRL4D controller, along with additional control options.
Dimensions: 204 x 25.5 x 136 mm / 8.03 x 1.0 x 5.35 in. Weight: 0.631 Kg / 1.391 lb.
	901,98 €
	1 145,51 €
	365 300 Ft
	463 931 Ft




	NEW!
	CVEOXRI4D
	VEO-XRI4D
	Control module for and expanded management experience with in-built WEB configuration interface. Dimensions 204 x 21.5 x 98.5mm / 4.7 x 0.85 x 3.88 in. Weight
0.540 Kg / 1.19 lb
	351,36 €
	446,22 €
	142 300 Ft
	180 721 Ft


HDBASET
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	NEW!
	CVEOXPT412
	VEO-XPT412
	VEO-XPT412 is a professional HDBaseT extension kit that includes both a transmitter and a receiver. Its 18 Gbps HDMI connectors allow for the extension of 4K video signals at 60Hz 4:4:4 up to 120 meters, or Full HD signals up to 150 meters, over a single Cat 5e or higher cable. Dimensions TBC. Weight: TBC
	500,74 €
	635,94 €
	202 800 Ft
	257 556 Ft



	CVEOXPT44A	VEO-XPT44A	VEO-XPT44A allows to extend a 4K video signal up to 40m or a Full HD signal up to 70m over a single	474,57 €
Cat 5e/6 cable. It supports 4K video signals at 60Hz with 4:4:4 YUV chroma subsampling and HDR10. The transmitter includes a HDMI loop output for monitoring or daisy-chain connection. A stereo unbalanced output on Euroblock connector is available both, on the transmitter and the receiver, for easy integration. In addition, VEO-XPT44A includes bidirectional PoH feature so the transmitter can be powered by the receiver and vice versa. With a reduced form factor and the added features of RS-232 and bidirectional IR, this is the perfect solution for any applications where AV and control extensions are required. Dimensions 154,4mm × 78,3mm × 20mm / 6.08“x 3.08“x 0.79“. Weight: 688g / 1.52lbs (Pair)
	602,70 €
	192 200 Ft
	244 094 Ft



	CVEOXTT44	VEO-XTT44	Ecler VEO-XTT44 is a professional HDBaseT Transmitter of High Dynamic Range (HDR) formats for	328,15 €
HDMI 2.0 extension. The extenders support video signal resolution up to 4K/UHD at 60Hz with 4:4:4 chroma sampling and HDMI data rate up to 18Gbps. Upscale fullHD input to 4K. Bidirectional PoH (Power Over HDBaseT) A 4-pin DIP switch allows managing EDID with multiple and customizable options. Include audio de-embedding and ARC support, bi-directional IR and RS-232 pass-through. A video pattern generator is included for testing purposes during the installation.
Dimensions (WxHxD) 140mm × 84mm × 20mm / 5.51“ x 3.31” x 0.79“ Weight 275g / 0,606 lb
	416,75 €
	132 900 Ft
	168 783 Ft



	CVEOXRT44	VEO-XRT44	Ecler VEO-XRT44 is a professional HDBaseT Receiver of High Dynamic Range (HDR) formats for HDMI	328,15 €
2.0 extension. The extenders support video signal resolution up to 4K/UHD at 60Hz with 4:4:4 chroma sampling and HDMI data rate up to 18Gbps. The scaler implemented in the TX allows to upscale fullHD input to 4K. Bidirectional PoH (Power Over HDBaseT) . A 4-pin DIP switch allows managing EDID with multiple and customizable options. The extenders include audio de-embedding and ARC support, bi- directional IR and RS-232 pass-through
Dimensions (WxHxD) 140mm × 84mm × 20mm / 5.51“ x 3.31” x 0.79“
Weight 290g / 0,640 lb
	416,75 €
	132 900 Ft
	168 783 Ft



	CVEOXWT44E	VEO-XWT44E	Ecler VEO-XWT44 is a HDbaseT transmitter in European 2-gang wallplate format. It allows to extend	776,54 €
one 4K video signal up to 40m over a single Cat 5e/6 cable or a FullHD signal up to 70m when connected to VEO-XRT44. It supports real 4K video signals at 60Hz with 4:4:4 YUV chroma subsampling and HDR 10 with a maximum bandwidth of 18Gbps. With bidirectional PoC feature, the transmitter can be powered by the receiver and vice versa. VEO-XWT44 includes 2 HDMI 2.0 Inputs and one USB-C Input selectable via front panel button, automatic switching feature or RS-232. It allows extending IR and a bidirectional RS-232 signal along with the video signal. Dimensions(WxHxD) 146mm × 86mm × 42mm / 5.75” x 3.39” x 1.65”. Weight 294g / 0.648 lbs
	986,21 €
	314 500 Ft
	399 415 Ft


HDMI
Nettó lista ár  Bruttó lista  Nettó lista ár  Bruttó lista ár
EUR	ár EUR	HUF	HUF


	CVEOXPS43	VEO-XPS43	VEO-XPS43 is a professional HDMI extender kit that delivers 4K@30Hz up to 30m and a 1080p@60Hz	149,63 €
up to 60m HDMI video extension over a single Cat. 6 cable or higher, with zero-latency, and 480i/480p/720p/1080i/1080p/UHD/4K resolution support. It includes unidirectional PoC (the receiver powered by the transmitter) and EDID management features as well as IR pass through, from the display to the source, for seamless integration. The transmitter also includes a HDMI loop output useful when integrating local displays and/or cascading to multiple devices.
Dimensions 79.5mm x 69mm x 16.5mm (3.13”x2.71”x0.65”) Weight TX: 132g / 0.291lbs, RX: 130g /
0.286 lbs
	190,03 €
	60 600 Ft
	76 962 Ft



	NEW!
	CVEOXPS47
	VEO-XPS47
	VEO-XPS47 is an HDMI 18Gbps extender kit that includes both a transmitter and a receiver. It enables 4K 50Hz 4:4:4 video signals to be extended up to 70 meters with zero latency over a single Cat 5e or higher cable.
Dimensions TBC Weight TBC.
	235,80 €
	299,47 €
	95 500 Ft
	121 285 Ft



	AUDIO MANAGEMENT DEVICES	
Nettó lista ár Bruttó lista  Nettó lista ár  Bruttó lista ár EUR	ár EUR	HUF	HUF


	CVEOAXS4	VEO-AXS4	The VEO-AXS4 allows to extract audio signals from HDMI signals up to 4K. It provides a stereo analog	122,47 €
output on RCA connectors or a 5.1 digital output on Toslink connector, selectable through the onboard switch.
Dimensions (WxHxD) 105mm x 29mm x 65mm / 4.13” x 2.56” x 1.14” Weight 175g / 0.39 lb
	155,54 €
	49 600 Ft
	62 992 Ft




	CVEOAXS4P	VEO-AXS4P	Ecler VEO-AXS4P is a professional HDMI audio extractor that allows to de-embed audio from a HDMI	153,58 €
signal, including audio from 4K sources. VEO-AXS4P provides uncompressed LPCM analogue stereo signal through RCA and Phoenix balanced output as well as Dolby Digital and DTS multichannel signals through the coaxial S/PDIF digital output. VEO-AXS4P is HDCP 2.2 and HDMI 2.0 compliant, supporting data rates up to 18 Gbps and video resolutions up to 4K/60Hz with 4:4:4 chroma sample and HDR contents.
Dimensions (WxHxD) 21.5 x 77 x 129 mm / 0.85” x 3.03” x 5.08”
Weight 244 g / 0.538 lb
	195,05 €
	62 200 Ft
	78 994 Ft



	CVEOAEXS4	VEO-AEXS4	VEO-AEXS4 allows to extract audio signals from HDMI streams up to 4K or to embed a stereo analogue	132,59 €
signal into the HDMI, replacing the original sound. It provides a stereo unbalanced analogue input and output on Euroblock connectors, or a 5.1 digital output on S/PDIF coaxial connector. Function mode is selectable through the onboard dip-switch. Dimensions: 104.4 x 89 x 28.3mm (4.11 x 3.5x 1.11 inches). Weight: 155g / 0,342 lb
	168,39 €
	53 700 Ft
	68 199 Ft



	CVEODACS4	VEO-DACS4	VEO-DACS4 allows to convert a digital audio signals from HDMI ARC inputs, S/PDIF Toslink or Coaxial,	101,48 €
to a stereo analogue signal. In addition it can be used to convert digital S/PDIF audio from Toslink to Coaxial and vice versa. It provides a stereo balanced analogue output on Euroblock connectors, and RCA. Function mode is selectable through the onboard switch. Dimensions: 96.2 x 47.6 x 21mm ( 3.79 x 1.87 x 0.83 inches). Weight: 155 g (0.309 lbs)
	128,88 €
	41 100 Ft
	52 197 Ft


AV INTERFACES
Nettó lista ár Bruttó lista  Nettó lista ár  Bruttó lista ár EUR	ár EUR	HUF	HUF



	CVEOCAP4U	VEO-CAP4U	VEO-CAP4U is a plug-n-play HDMI to USB video capture device aimed for online media creators,	245,93 €
schools,educational and corporate market etc. that require a professional solution for capturing and streaming their audiovisual content. This product is designed to easily record video and audio from an HDMI source, and send it to a PC / MAC over USB 3.0 without the need of an external power supply or installation drivers. A balanced line input automatically mixes an external sound source into the main audio stream. Dimensions: 102mm × 68mm × 12mm (4.02” x 2.68” x 0.59”). Weight: 75g / 0.165 lbs
	312,33 €
	99 600 Ft
	126 492 Ft


ACCESSORIES
Nettó lista ár Bruttó lista  Nettó lista ár  Bruttó lista ár EUR	ár EUR	HUF	HUF



	CVEORACK19	VEO-RACK19	Univ. 19” Rack mount shelf VEO series. Includes 12 x M3 screws with nuts and Dual Lock™ tape for	101,48 €
devices not provided of mounting ears. Central holes for cable ties.
	128,88 €
	41 100 Ft
	52 197 Ft



	NEW!
	CVEORK1CG2
	VEO-RK1CG2
	VEO-RK1CG2 rack mount shelf is specifically designed for the VEO-1CG2 series, targeting the professional video market. Its 3U/19” frame supports both front and rear orientations for the mounted devices, enhancing its versatility across different setups. This shelf comes equipped with brackets and screws, enabling the installation of up to 12 VEO-XTI1CG2 or VEO-XRI1CG2 units. Dimensions: 483x132x15 mm / 19.02 x 5.20 x 0.59 in., Weight: 1.32 kg / 2.92 lb.
	175,80 €
	223,27 €
	71 200 Ft
	90 424 Ft



	CVEOCH200	VEO-CH200	VEO-CH200 is a high speed HDMI 2.0 cable with Ethernet.	7,16 €
These high quality cables are the perfect solution for professional installations, ensuring reliable and seamless HDMI 2.0 connections up to 18Gbps.
All cables support HDMI, Ethernet, Audio and Control (ARC and CEC) signals. Length: 0.5m
	9,09 €
	2 900 Ft
	3 683 Ft



	CVEOCH201	VEO-CH201	VEO-CH201 is a high speed HDMI 2.0 cable with Ethernet.	9,14 €
These high quality cables are the perfect solution for professional installations, ensuring reliable and seamless HDMI 2.0 connections up to 18Gbps.
All cables support HDMI, Ethernet, Audio and Control (ARC and CEC) signals. Length: 1m
	11,60 €
	3 700 Ft
	4 699 Ft



	CVEOCH202	VEO-CH202	VEO-CH202 is a high speed HDMI 2.0 cable with Ethernet.	12,10 €
These high quality cables are the perfect solution for professional installations, ensuring reliable and seamless HDMI 2.0 connections up to 18Gbps.
All cables support HDMI, Ethernet, Audio and Control (ARC and CEC) signals. Length: 2m
	15,37 €
	4 900 Ft
	6 223 Ft



	CVEOCH203	VEO-CH203	VEO-CH203 is a high speed HDMI 2.0 cable with Ethernet.	16,30 €
These high quality cables are the perfect solution for professional installations, ensuring reliable and seamless HDMI 2.0 connections up to 18Gbps.
All cables support HDMI, Ethernet, Audio and Control (ARC and CEC) signals. Length: 3m
	20,70 €
	6 600 Ft
	8 382 Ft



	CVEOCH205	VEO-CH205	VEO-CH205 is a high speed HDMI 2.0 cable with Ethernet.	21,23 €
These high quality cables are the perfect solution for professional installations, ensuring reliable and seamless HDMI 2.0 connections up to 18Gbps.
All cables support HDMI, Ethernet, Audio and Control (ARC and CEC) signals. Length: 5m
	26,97 €
	8 600 Ft
	10 922 Ft





	CVEOCH208	VEO-CH208	VEO-CH208 is a high speed HDMI 2.0 cable with Ethernet.	36,30 €
These high quality cables are the perfect solution for professional installations, ensuring reliable and seamless HDMI 2.0 connections up to 18Gbps.
All cables support HDMI, Ethernet, Audio and Control (ARC and CEC) signals. Length: 8m
	46,10 €
	14 700 Ft
	18 669 Ft



	CVEOCH210	VEO-CH210	VEO-CH210 is a high speed HDMI 2.0 cable with Ethernet.	54,32 €
These high quality cables are the perfect solution for professional installations, ensuring reliable and seamless HDMI 2.0 connections up to 18Gbps.
All cables support HDMI, Ethernet, Audio and Control (ARC and CEC) signals. Length: 10m
	68,99 €
	22 000 Ft
	27 940 Ft



	NEW!
	CVEOXCH415

[image: ]
	VEO-XCH415
	VEO-XCH415 is a 15m 48 Gbps professional-grade Active Optical HDMI® Cable (AOC) designed to complement Ecler’s video product range. This high-performance cable ensures a reliable and seamless unidirectional HDMI® connection, supporting up to 8K 60Hz 4:4:4 resolution, 48-bit Deep Colour, and HDR content. The durable PVC jacket provides flexibility and robustness while maintaining a sleek black design, making it ideal for professional installations that require long-distance, high-quality HDMI® connections.
	90,37 €
	114,77 €
	36 600 Ft
	46 482 Ft



	NEW!
	CVEOXCH430

[image: ]
	VEO-XCH430
	VEO-XCH415 is a 30m 48 Gbps professional-grade Active Optical HDMI® Cable (AOC) designed to complement Ecler’s video product range. This high-performance cable ensures a reliable and seamless unidirectional HDMI® connection, supporting up to 8K 60Hz 4:4:4 resolution, 48-bit Deep Colour, and HDR content. The durable PVC jacket provides flexibility and robustness while maintaining a sleek black design, making it ideal for professional installations that require long-distance, high-quality HDMI® connections.
	120,49 €
	153,03 €
	48 800 Ft
	61 976 Ft



	NEW!
	CVEOXCH450

[image: ]
	VEO-XCH450
	VEO-XCH415 is a 50m 48 Gbps professional-grade Active Optical HDMI® Cable (AOC) designed to complement Ecler’s video product range. This high-performance cable ensures a reliable and seamless unidirectional HDMI® connection, supporting up to 8K 60Hz 4:4:4 resolution, 48-bit Deep Colour, and HDR content. The durable PVC jacket provides flexibility and robustness while maintaining a sleek black design, making it ideal for professional installations that require long-distance, high-quality HDMI®
connections.
	155,56 €
	197,56 €
	63 000 Ft
	80 010 Ft



	NEW!
	CVEOXCH470

[image: ]
	VEO-XCH470
	VEO-XCH415 is a 70m 48 Gbps professional-grade Active Optical HDMI® Cable (AOC) designed to complement Ecler’s video product range. This high-performance cable ensures a reliable and seamless unidirectional HDMI® connection, supporting up to 8K 60Hz 4:4:4 resolution, 48-bit Deep Colour, and HDR content. The durable PVC jacket provides flexibility and robustness while maintaining a sleek black design, making it ideal for professional installations that require long-distance, high-quality HDMI®
connections.
	190,62 €
	242,08 €
	77 200 Ft
	98 044 Ft
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